================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述:
此样例是通过轮询方式对串口外设接口（SPI）与外部设备以全双工串行方式进行通信的演
示。主设备提供通信时钟SCK，通过MOSI/MISO引脚发送/接收数据。从设备通过MOSI/MISO引
脚接收/发送数据。数据以主机提供的SCK沿同步被移位，完成全双工通信。

Function descriptions:
This sample is a demonstration of the Serial Peripheral Interface (SPI) 
communicating with an external device in full-duplex serial mode by polling. 
The master device provides the communication clock SCK and sends/receives data 
via the MOSI/MISO pin. The slave device receives/transmits data through the 
MOSI/MISO pins. The data is shifted synchronously along the SCK provided by the 
master to complete full-duplex communication.

================================================================================
测试环境：
测试用板：PY32F005_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F005_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤:
1.选择两块PY32F005_STK板，一块作为主机，一块作为从机
2.编译下载主机程序SPI_TwoBoards_FullDuplexMaster_Polling_Init
3.编译下载从机程序SPI_TwoBoards_FullDuplexSlave_Polling_Init
4.主机与从机引脚连接(箭头指向为信号传输方向) 
主机MASTER：         从机SLAVE：
SCK(PB0)   ----->    SCK(PB0)
MISO(PB2)  <-----    MISO(PB2)
MOSI(PB3)  ----->    MOSI(PB3)
NSS(PB1)   ----->    NSS(PB1)
GND       <----->    GND
5.主从机上电
6.按下从机复位按键先运行从机程序，再按下主机用户按键运行主机程序 
7.观察主从机的LED灯，当主机和从机LED灯由常暗转为常亮状态，则表明主机、从机收发数
据成功；当主机或从机LED灯处于闪烁状态，则表明主机、从机收发数据失败。

Example execution steps:
1.Select two PY32F005 blocks_ STK board, one as the master and one as the slave
2.Compile and download master program SPI_TwoBoards_FullDuplexMaster_Polling_Init
3.Compile and download slave program SPI_TwoBoards_FullDuplexSlave_Polling_Init
4.Connection between the master and slave pins (arrow pointing in the direction
of signal transmission)
MASTER：             SLAVE：
SCK(PB0)   ----->    SCK(PB0)
MISO(PB2)  <-----    MISO(PB2)
MOSI(PB3)  ----->    MOSI(PB3)
NSS(PB1)   ----->    NSS(PB1)
GND       <----->    GND
5.Powering on the master and slave machines
6.Press the slave reset button to run the slave program first, and then press
the master user button to run the master program
7.Observe the LED lights of the master and slave machines. When the LED lights
of the master and slave machines change from normally dark to normally on, it
indicates that the master and slave machines have successfully transmitted and
received data; When the LED light of the master or slave is in a flashing state,
it indicates that the master or slave has failed to transmit and receive data.
================================================================================
注意事项:
1.必须先按从机复位按键使从机程序先运行，再按主机用户按键开始运行主机程序，否则会
导致主从机通信失败。
2.NSS引脚只需要在使用NSS硬件方式时连接（本样例使用的是NSS硬件方式）

Notes:
1.You must first press the slave reset button to run the slave program first,
and then press the master user button to start running the master program, otherwise
it will cause communication failure between the master and slave machines.
2.The NSS pin only needs to be connected when using NSS hardware mode
(this example uses NSS hardware mode)
3.The LED light pin on the board is PA1, which matches the SPI_ The MISO pins
================================================================================