================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了TIM1的三通道异或输入捕获功能。配置PA8、PA9、PA10为通道1、通道2、通道3
的输入引脚。每当有一个引脚电平变化时会触发捕获中断，并在中断处理中翻转LED。

Function descriptions:
This sample demonstrates the XOR input capture functionality of TIM1 using three 
channels: PA8, PA9, and PA10 as the input pins for channel 1, channel 2, and 
channel 3, respectively. Whenever there is a change in the level of any of the 
input pins, it triggers the capture interrupt and toggles the LED in the 
interrupt handler.
================================================================================
测试环境：
测试用板：PY32F031_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F031_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行
2. PA8/PA9/PA10保持任意两个引脚电平不变，当剩下一引脚电平变化时LED翻转

Example execution steps:
1.Compile and download the program to the MCU, and then run it.
2.Keep the level of any two pins(PA8/PA9/PA10) unchanged, and when the level of the 
remaining pin changes, the LED will toggle.
================================================================================
注意事项：

Notes:

================================================================================