================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了ADC的模拟看门狗功能，当开启看门狗的通道的电压值不在设定的上下限中，
会进入看门狗中断。

Function descriptions:
This example demonstrates the analog watchdog function of ADC. When the voltage
value of the channel that opens the watchdog is not within the set upper or 
lower limits,Will enter watchdog interrupt.
================================================================================
测试环境：
测试用板：PY32F031_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F031_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. PA4的电压值小于1.65V(供电电压为3.3V),不会进入看门狗中断，LED灯不亮；
3. PA4的电压值大于1.65V(供电电压为3.3V)，进入看门狗中断，LED亮。

Example execution steps:
1. Compile and download the program to MCU and run it;
2. If the voltage value of PA4 is less than 1.65V (with a power supply voltage of
3.3V), it will not enter the watchdog interrupt and the LED light will not light 
up;
3. If the voltage value of PA4 is greater than 1.65V (with a supply voltage of 
3.3V), the watchdog will interrupt and the LED will light up.
================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下:
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required
Connect PC and STK board through USB to TTL module and the connection method
is as follows
@PrintfConfigStart
STK board    USB to TTL moudle
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND      -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================