================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了stop模式下，通过GPIO中断唤醒功能。

Function descriptions:
This sample demonstrates the stop mode with GPIO interrupt wake-up feature.
================================================================================
测试环境：
测试用板：PY32F071_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F071_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. LED灯亮，按下按键，LED灯灭，串口打印"STOP MODE!"，进入stop模式；
3. 在PA06上产生一个下降沿，程序退出stop模式，并且串口打印"WAKEUP OK!"；
4. LED以200ms的间隔进行翻转。

Example execution steps:
1. Compile and download the program to the MCU and run it.
2. The LED is on, press the button, the LED turns off, and "STOP MODE!" is 
   printed on the serial port, entering the stop mode.
3. Generate a falling edge on PA06 to wake up the program from stop mode, and 
   "WAKEUP OK!" will be printed on the serial port.
4. The LED will toggle with an interval of 200ms.
================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

1. 演示此样例功能时需要断开swd连接线并重新上电，因为默认情况下，仿真器会把
   DBGMCU_CR.DBG_STOP置位。
2. 注意关闭systick中断，防止该中断唤醒MCU。

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required
Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
@PrintfConfigStart
STK board USB to TTL module
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd

1. When demonstrating this sample, it is necessary to disconnect the SWD 
   connection and power on again because the debugger will set 
   DBGMCU_CR.DBG_STOP by default.
2. Pay attention to disable the systick interrupt to prevent it from waking 
   up the MCU.
================================================================================
