================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了采用CAN2.0协议标准帧轮询方式与PCAN-View的通信功能，MCU首先自动向
PCAN-View发送8byte数据0x1~0x8，PCAN-View接收到数据后，然后手动通过PCAN-View向MCU
发送ID为0x12F的8byte数据，MCU会自动将接收到数据通过串口打出。

Function descriptions:
This example demonstrates the communication function with PCAN View using the
CAN2.0 protocol standard frame polling method. The MCU first automatically sends
8-byte data 0x1~0x8 to PCAN View. After PCAN View receives the data, it manually
sends 8-byte data with ID 0x12F to the MCU through PCAN View. The MCU will
automatically print the received data through the serial port.
================================================================================
测试环境：
测试用板：PY32F072_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F072_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译并下载程序；
2. 通过USB转CAN模块连接PC、CAN转接板、STK板,连线方式如下；
STK板               CAN转接板
PB8(CAN_RX)  -->    R21  
PB9(CAN_TX)  -->    R20
GND           -->    GND

CAN转接板           USB转CAN模块
CAN-H         -->    CAN-H
CAN-L         -->    CAN-L
3. 打开PCAN-View，配置PCAN-View连接方式为：CAN2.0，Clock Frequency：24MHz，
Nominal Bit Rate：250kBit/s，Data Bit Rate：不设置，Standard
4. 复位STK板，观察PCAN-View是否接收到8byte数据数据0x1~0x8，PCAN-View接收到表明
STK板发送数据成功，否则表明STK板发送数据失败；
5. PCAN-View接收到数据后，手动通过PCAN-View发送ID为0x12F的8byte数据，观察串口是
否打印PCAN-View发送的数据，如果串口打印，表明STK板接收数据成功，否则STK板接收数
据失败。

Example execution steps:
1.Compile and download the program;
2.Connect the PC, CAN adapter board, and STK board through the USB to CAN module,
and the connection method is as follows:
STK board           CAN adapter board
PB8(CAN_RX)    -->    R21  
PB9(CAN_TX)    -->    R20
GND            -->    GND

CAN adapter board     USB to CAN module
CAN-H           -->    CAN-H
CAN-L           -->    CAN-L
3.Open PCAN-View and configure the connection method for PCAN-View as CAN2.0,
Clock Frequency: 24MHz, Nominal Bit Rate: 250kBit/s, Data Bit Rate: not set,
Standard
4.Reset the STK board and observe if PCAN-View has received 8-byte data data
0x1~0x8. PCAN-View receiving indicates that the STK board has successfully sent
data, otherwise it indicates that the STK board has failed to send data;
5.After receiving the data, PCAN-View manually sends an 8-byte data with ID
0x12F through PCAN-View. Observe whether the serial port prints the data sent
by PCAN-View. If the serial port prints, it indicates that the STK board has
successfully received the data, otherwise the STK board has failed to receive
the data.
================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required
Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
@PrintfConfigStart
STK board USB to TTL module
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================