================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了COMP比较器唤醒功能，PD0作为比较器正端输入，1/2VCC作为比较器负端输
入，进入stop模式后，通过调整PD0上的输入电压，产生中断唤醒stop模式。

Function descriptions:
This example demonstrates the COMP comparator wake-up function, with PD0 as the
positive input and 1/2VCC as the negative input of the comparator. After
entering stop mode, the interrupt wake-up stop mode is generated by adjusting
the input voltage on PD0.

================================================================================
测试环境：
测试用板：PY32F092_STK
MDK版本： 5.28
IAR版本： 9.20
GCC版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F092_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. LED亮起后按下按键，进入stop模式，LED熄灭；
3. 在PD0上输入从小于1.6V到的大于1.7V电压时，产生中断唤醒；
4. 接下来LED每隔200ms进行翻转，程序正常运行。

Example execution steps:
1.Compile and download the program to MCU and run it;
2.After the LED lights up, press the button to enter the stop mode, and the
LED goes out;
3. An interrupt wake-up is generated when a voltage greater than 1.7V from less
than 1.6V is input to PD0;;
4. Next, the LED flips every 200ms and the program runs normally
================================================================================
注意事项：

Notes:
================================================================================