================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了ADC模块的软件触发和轮询功能。

Function descriptions:
This example demonstrates the software triggering and polling functions of the
ADC module.
================================================================================
测试环境：
测试用板：PY32MD420_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32MD420_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 串口每隔1s打印一次通道4(PA4)的DR值。

Example execution steps:
1. Compile and download the program and run it;
2. The serial port prints the DR value of channel 4 (PA4) every 1 second.
================================================================================
注意事项：
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下:
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
Connect PC and STK board through USB to TTL module and the connection method
is as follows
@PrintfConfigStart
STK board    USB to TTL moudle
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND      -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================