================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了SCI的自动波特率检测功能,上位机发送1字节的波特率检测字符0x55，如果
MCU检测成功，则返回字符：Auto BaudRate Test。

Function descriptions:
This example demonstrates the automatic baud rate detection function of SCI.
If the MCU detects successfully after the upper computer sends 1 byte baud rate
detection character 0x55, it will returns the string: Auto BaudRate Test.
================================================================================
测试环境：
测试用板：PY32MD530_STK
MDK版本： 5.28

Test environment:
Test board: PY32MD530_STK
MDK Version: 5.28
================================================================================
使用步骤：
1. 编译并下载程序到MCU；
2. 通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
STK板         USB转TTL模块
PA2(TX)   --> RX
PA3(RX)   --> TX
GND       --> GND
3. PC端打开串口调试助手，正确连接上通讯COM口，波特率设置为9600。
4. 调试助手发送一个字符0x55，MCU反馈字符串：Auto BaudRate Test；

Example execution steps:
1. compile and download the program to MCU and run it;
2. Connect the PC to the STK board through the USB-to-TTL module. The connection 
method between the STK board and the USB-to-TTL module is as follows.
STK board     USB-to-TTL module
PA2(TX)   --> RX
PA3(RX)   --> TX
GND       --> GND
3. Open the serial port Assistant on the PC, connect the COM port correctly, and
set the baud rate to 9600.
4. Send a character 0x55 using the serial assistant. The MCU will return the 
string "Auto BaudRate Test".
================================================================================
注意事项：

Notes:

================================================================================