================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了主机I2C通过DMA方式进行通讯，从机使用EEPROM外设芯片P24C32，按下user按
键，主机先向从机写15bytes数据为0x1~0xf，然后再从EEPROM中将写入的数据读出，读取成
功后，主机板上的小灯处于“常亮”状态。

Function descriptions:
This sample demonstrates the host I2C communication through DMA, the slave using
EEPROM peripheral chip P24C32, press the user button, the host first to the slave
to write 15bytes of data for the 0x1 ~ 0xf, and then from the EEPROM will be
written to read out the data, read the success of the host board, the small light
is in the “always on” state! After successful reading, the small light on the
host board is in “always on” state.
================================================================================
测试环境：
测试用板：PY32MD550_STK
MDK版本： 5.28

Test environment:
Test board: PY32MD550_STK
MDK Version: 5.28
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 先复位从机，然后再复位主机；
3. 复位完成后，按下主机user按键，先写15bytes数据0x1-0xf；
4. 延时100ms后，从eeprom读取15bytes数据；
5. 观察主机的LED灯，当主机LED灯由常暗转为常亮状态，则表明主机收发数据成功；当
主机LED灯处于闪烁状态，则表明主机收发数据失败。

Example execution steps:
1.Compile and download the program to the MCU and run it.
2.Reset the slave device first, then reset the master device.
3.After the reset is complete, press the user button on the master device to 
write 15 bytes of data ranging from 0x1 to 0xF to the slave device.
4.After a delay of 100 milliseconds, read 15 bytes of data from the EEPROM.
5.Observe the LED on the master board. If the LED transitions from constantly 
dim to constantly lit, it indicates successful data transmission and reception 
by the master. If the LED is blinking, it indicates data transmission or 
reception failure.
================================================================================
注意事项：
PA8  -------> I2C1_SCL
PA7  -------> I2C1_SDA
如需修改速率，直接修改I2C_SPEEDCLOCK即可。

Notes:
PA8  -------> I2C1_SCL
PA7  -------> I2C1_SDA
To modify the rate, modify I2C_SPEEDCLOCK directly.
================================================================================