================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
定时器1的使能由定时器2控制，当定时器2计数时，LED会常亮，当定时器2发生更新事件时，
更新事件会触发定时器1，定时器1开始计数后，LED会以5Hz的频率进行翻转

Function descriptions:
The enable of TIM1 is controlled by TIM2. When TIM2 counts, the LED will be 
steady on. The update event generated by TIM2 will triggers TIM1, and when TIM1 
starts counting, the LED is toggled at a frequency of 5Hz
================================================================================
测试环境：
测试用板：PY32T090_STK
MDK版本： 5.28
IAR版本： 9.20
GCC版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32T090_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 下载程序并运行；
2. 运行程序，在仿真模式下查看，TIM1先不会计数,当TIM2发生更新事件后，
TIM1开始计数
3. TIM1开始计数后，LED会以5Hz的频率进行翻转

Example execution steps:
1. compile and download the program to MCU and run it;
2. Run the program and check it in debug mode. TIM1 will not count first.
After an update event occurs in TIM2,TIM1 starts counting
3. After TIM1 starts counting, the LED will flip at a frequency of 5Hz
================================================================================
注意事项：
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
@PrintfConfigStart
STK板        USB转TTL模块
PB9(TX)   -->  RX
PB8(RX)   -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
@PrintfConfigStart
STK board USB to TTL module
PB9(TX)   -->  RX
PB8(RX)   -->  TX
GND       -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================