================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了ADC模块的VREFINT采样功能，通过采样VREFINT的值，计算得出VCC的值，并通过
串口打印出来。

Function descriptions:
This example demonstrates the VREFINT sampling function of the ADC module. By
sampling the value of VREFINT, the VCC value is calculated and printed through
the serial port.
================================================================================
测试环境：
测试用板：PY32F031_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F031_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译并下载程序；
2. 串口每隔1s打印一次VCC的电压值。

Example execution steps:
1. Compile and download the program;
2. The serial port prints the voltage value of VCC every 1 second.
================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下:
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required
Connect PC and STK board through USB to TTL module and the connection method
is as follows
@PrintfConfigStart
STK board    USB to TTL moudle
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND      -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================