================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了FreeRTOS三个任务依照优先级大小依次切换的实验。通过串口log，观察任务
切换顺序。

Function descriptions:
This sample demonstrates an experiment in which three FreeRTOS tasks are 
switched in order of priority. Observe the switching order through the serial 
port log.

================================================================================
测试环境：
测试用板：PY32F040E_STK
MDK版本：5.28
IAR版本：9.20
GCC版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F040E_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 通过串口调试助手打印的log信息，观察任务执行过程。
   任务执行顺序为：Task3->Task2->Task1
   Task1: 打印"Task1 is running"信息。
   Task2: 打印"Task2 is running"信息。
   Task3: 打印"Task3 is running"信息。

Example execution steps:
1. Compile and download the program to the MCU and run it;
2. You can use the log information printed by the serial debugging assistant to 
observe the task execution process.
   Task execution sequence: Task3->Task2->Task1
   Task1: Print the "Task1 is running" message.
   Task2: Print the "Task2 is running" message.
   Task3: Print the "Task3 is running" message.

================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作
通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
@PrintfConfigStart
STK板        USB转TTL模块
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART配置为波特率115200，数据位8，停止位1，校验位None
@PrintfConfigEnd

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required
Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
@PrintfConfigStart
STK board USB to TTL module
PA02(TX)  -->  RX
PA03(RX)  -->  TX
GND       -->  GND
UART is configured as BaudRate 115200, data bit 8, stop bit 1, and parity None.
@PrintfConfigEnd
================================================================================
