================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了sleep模式下，GPIO外部中断唤醒功能。

Function descriptions:
This sample demonstrates the GPIO external interrupt wake-up feature in sleep 
mode. When the program starts running, the LED will be on. Press the button, 
and the LED will turn off, entering sleep mode. When a falling edge is detected 
on PA06, the program will exit sleep mode. The LED will toggle at intervals 
of 500ms.

================================================================================
测试环境：
测试用板：PY32F403_STK
MDK版本：5.28
IAR版本：9.20
GCC版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F403_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10

================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. LED灯亮，按下按键，LED灯灭，进入sleep模式；
3. 在PA06上产生一个下降沿，程序退出sleep模式；
4. LED以500ms的间隔进行翻转。

Example execution steps:
1. Compile and download the program to the MCU and run it;
2. The LED will be on initially. Press the button, and the LED will turn off, 
   entering sleep mode;
3. Generate a falling edge on PA06, and the program will exit sleep mode;
4. The LED will toggle at intervals of 500ms.

================================================================================
注意事项：
如果需要使用按键:
StartKit版本为V2.0以下,需将StartKit.h中的StartKitVersion 2 注释掉，并打开
StartKitVersion 1
StartKit版本为V2.0及以上版本,则无需操作

Notes:
If you need to use buttons:
StartKit version is below V2.0, you need to comment StartKitVersion 2 in
StartKit.h, and open StartKitVersion 1 
StartKit version is V2.0 and above, no operation is required

================================================================================
