<?xml version="1.0" encoding="UTF-8"?>

<package schemaVersion="1.3" xmlns:xs="http://www.w3.org/2001/XMLSchema-instance" xs:noNamespaceSchemaLocation="PACK.xsd">
  <name>CMSIS</name>
  <description>CMSIS (Cortex Microcontroller Software Interface Standard)</description>
  <vendor>ARM</vendor>
  <!-- <license>license.txt</license> -->
  <url>http://www.keil.com/pack/</url>

  <releases>
    <release version="5.4.0" date="2018-08-01">
      Aligned pack structure with repository.
      The following folders are deprecated:
        - CMSIS/Include/
        - CMSIS/DSP_Lib/

      CMSIS-Core(M): 5.1.2 (see revision history for details)
        - Added Cortex-M1 support (beta).
      CMSIS-Core(A): 1.1.2 (see revision history for details)
      CMSIS-NN: 1.1.0
        - Added new math functions.
      CMSIS-RTOS2:
        - API 2.1.3 (see revision history for details)
        - RTX 5.4.0 (see revision history for details)
          * Updated exception handling on Cortex-A
      CMSIS-Driver:
        - Flash Driver API V2.2.0
      Utilities:
        - SVDConv 3.3.21
        - PackChk 1.3.71
    </release>
    <release version="5.3.0" date="2018-02-22">
      Updated Arm company brand.
      CMSIS-Core(M): 5.1.1 (see revision history for details)
      CMSIS-Core(A): 1.1.1 (see revision history for details)
      CMSIS-DAP: 2.0.0 (see revision history for details)
      CMSIS-NN: 1.0.0
        - Initial contribution of the bare metal Neural Network Library.
      CMSIS-RTOS2:
        - RTX 5.3.0 (see revision history for details)
        - OS Tick API 1.0.1
    </release>
    <release version="5.2.0" date="2017-11-16">
      CMSIS-Core(M): 5.1.0 (see revision history for details)
        - Added MPU Functions for ARMv8-M for Cortex-M23/M33.
        - Added compiler_iccarm.h to replace compiler_iar.h shipped with the compiler.
      CMSIS-Core(A): 1.1.0 (see revision history for details)
        - Added compiler_iccarm.h.
        - Added additional access functions for physical timer.
      CMSIS-DAP: 1.2.0 (see revision history for details)
      CMSIS-DSP: 1.5.2 (see revision history for details)
      CMSIS-Driver: 2.6.0 (see revision history for details)
        - CAN Driver API V1.2.0
        - NAND Driver API V2.3.0
      CMSIS-RTOS:
        - RTX: added variant for Infineon XMC4 series affected by PMU_CM.001 errata.
      CMSIS-RTOS2:
        - API 2.1.2 (see revision history for details)
        - RTX 5.2.3 (see revision history for details)
      Devices:
        - Added GCC startup and linker script for Cortex-A9.
        - Added device ARMCM0plus_MPU for Cortex-M0+ with MPU.
        - Added IAR startup code for Cortex-A9
    </release>
    <release version="5.1.1" date="2017-09-19">
      CMSIS-RTOS2:
      - RTX 5.2.1 (see revision history for details)
    </release>
    <release version="5.1.0" date="2017-08-04">
      CMSIS-Core(M): 5.0.2 (see revision history for details)
      - Changed Version Control macros to be core agnostic.
      - Added MPU Functions for ARMv7-M for Cortex-M0+/M3/M4/M7.
      CMSIS-Core(A): 1.0.0 (see revision history for details)
      - Initial release
      - IRQ Controller API 1.0.0
      CMSIS-Driver: 2.05 (see revision history for details)
      - All typedefs related to status have been made volatile.
      CMSIS-RTOS2:
      - API 2.1.1 (see revision history for details)
      - RTX 5.2.0 (see revision history for details)
      - OS Tick API 1.0.0
      CMSIS-DSP: 1.5.2 (see revision history for details)
      - Fixed GNU Compiler specific diagnostics.
      CMSIS-Pack: 1.5.0 (see revision history for details)
      - added System Description File (*.SDF) Format
      CMSIS-Zone: 0.0.1 (Preview)
      - Initial specification draft
    </release>
    <release version="5.0.1" date="2017-02-03">
      Package Description:
      - added taxonomy for Cclass RTOS
      CMSIS-RTOS2:
      - API 2.1   (see revision history for details)
      - RTX 5.1.0 (see revision history for details)
      CMSIS-Core: 5.0.1 (see revision history for details)
      - Added __PACKED_STRUCT macro
      - Added uVisior support
      - Updated cmsis_armcc.h: corrected macro __ARM_ARCH_6M__
      - Updated template for secure main function (main_s.c)
      - Updated template for Context Management for ARMv8-M TrustZone (tz_context.c)
      CMSIS-DSP: 1.5.1 (see revision history for details)
      - added ARMv8M DSP libraries.
      CMSIS-Pack:1.4.9 (see revision history for details)
      - added Pack Index File specification and schema file
    </release>
    <release version="5.0.0" date="2016-11-11">
      Changed open source license to Apache 2.0
      CMSIS_Core:
       - Added support for Cortex-M23 and Cortex-M33.
       - Added ARMv8-M device configurations for mainline and baseline.
       - Added CMSE support and thread context management for TrustZone for ARMv8-M
       - Added cmsis_compiler.h to unify compiler behaviour.
       - Updated function SCB_EnableICache (for Cortex-M7).
       - Added functions: NVIC_GetEnableIRQ, SCB_GetFPUType
      CMSIS-RTOS:
        - bug fix in RTX 4.82 (see revision history for details)
      CMSIS-RTOS2:
        - new API including compatibility layer to CMSIS-RTOS
        - reference implementation based on RTX5
        - supports all Cortex-M variants including TrustZone for ARMv8-M
      CMSIS-SVD:
       - reworked SVD format documentation
       - removed SVD file database documentation as SVD files are distributed in packs
       - updated SVDConv for Win32 and Linux
      CMSIS-DSP:
       - Moved DSP libraries from CMSIS/DSP/Lib to CMSIS/Lib.
       - Added DSP libraries build projects to CMSIS pack.
    </release>
    <release version="4.5.0" date="2015-10-28">
      - CMSIS-Core     4.30.0  (see revision history for details)
      - CMSIS-DAP      1.1.0   (unchanged)
      - CMSIS-Driver   2.04.0  (see revision history for details)
      - CMSIS-DSP      1.4.7   (no source code change [still labeled 1.4.5], see revision history for details)
      - CMSIS-Pack     1.4.1   (see revision history for details)
      - CMSIS-RTOS     4.80.0  Restored time delay parameter 'millisec' old behavior (prior V4.79) for software compatibility. (see revision history for details)
      - CMSIS-SVD      1.3.1   (see revision history for details)
    </release>
    <release version="4.4.0" date="2015-09-11">
      - CMSIS-Core     4.20   (see revision history for details)
      - CMSIS-DSP      1.4.6  (no source code change [still labeled 1.4.5], see revision history for details)
      - CMSIS-Pack     1.4.0  (adding memory attributes, algorithm style)
      - CMSIS-Driver   2.03.0 (adding CAN [Controller Area Network] API)
      - CMSIS-RTOS
        -- API         1.02   (unchanged)
        -- RTX         4.79   (see revision history for details)
      - CMSIS-SVD      1.3.0  (see revision history for details)
      - CMSIS-DAP      1.1.0  (extended with SWO support)
    </release>
    <release version="4.3.0" date="2015-03-20">
      - CMSIS-Core     4.10   (Cortex-M7 extended Cache Maintenance functions)
      - CMSIS-DSP      1.4.5  (see revision history for details)
      - CMSIS-Driver   2.02   (adding SAI (Serial Audio Interface) API)
      - CMSIS-Pack     1.3.3  (Semantic Versioning, Generator extensions)
      - CMSIS-RTOS
        -- API         1.02   (unchanged)
        -- RTX         4.78   (see revision history for details)
      - CMSIS-SVD      1.2    (unchanged)
    </release>
    <release version="4.2.0" date="2014-09-24">
      Adding Cortex-M7 support
      - CMSIS-Core     4.00  (Cortex-M7 support, corrected C++ include guards in core header files)
      - CMSIS-DSP      1.4.4 (Cortex-M7 support and corrected out of bound issues)
      - CMSIS-Pack     1.3.1 (Cortex-M7 updates, clarification, corrected batch files in Tutorial)
      - CMSIS-SVD      1.2   (Cortex-M7 extensions)
      - CMSIS-RTOS RTX 4.75  (see revision history for details)
    </release>
    <release version="4.1.1" date="2014-06-30">
      - fixed conditions preventing the inclusion of the DSP library in projects for Infineon XMC4000 series devices
    </release>
    <release version="4.1.0" date="2014-06-12">
      - CMSIS-Driver   2.02  (incompatible update)
      - CMSIS-Pack     1.3   (see revision history for details)
      - CMSIS-DSP      1.4.2 (unchanged)
      - CMSIS-Core     3.30  (unchanged)
      - CMSIS-RTOS RTX 4.74  (unchanged)
      - CMSIS-RTOS API 1.02  (unchanged)
      - CMSIS-SVD      1.10  (unchanged)
      PACK:
      - removed G++ specific files from PACK
      - added Component Startup variant "C Startup"
      - added Pack Checking Utility
      - updated conditions to reflect tool-chain dependency
      - added Taxonomy for Graphics
      - updated Taxonomy for unified drivers from "Drivers" to "CMSIS Drivers"
    </release>
    <release version="4.0.0">
      - CMSIS-Driver   2.00  Preliminary (incompatible update)
      - CMSIS-Pack     1.1   Preliminary
      - CMSIS-DSP      1.4.2 (see revision history for details)
      - CMSIS-Core     3.30  (see revision history for details)
      - CMSIS-RTOS RTX 4.74  (see revision history for details)
      - CMSIS-RTOS API 1.02  (unchanged)
      - CMSIS-SVD      1.10  (unchanged)
    </release>
    <release version="3.20.4">
      - CMSIS-RTOS 4.74 (see revision history for details)
      - PACK Extensions (Boards, Device Features, Flash Programming, Generators, Configuration Wizard). Schema version 1.1.
    </release>
    <release version="3.20.3">
      - CMSIS-Driver API Version 1.10 ARM prefix added (incompatible change)
      - CMSIS-RTOS 4.73 (see revision history for details)
    </release>
    <release version="3.20.2">
      - CMSIS-Pack documentation has been added
      - CMSIS-Drivers header and documentation have been added to PACK
      - CMSIS-CORE, CMSIS-DSP, CMSIS-RTOS API and CMSIS-SVD remain unchanged
    </release>
    <release version="3.20.1">
      - CMSIS-RTOS Keil RTX V4.72 has been added to PACK
      - CMSIS-CORE, CMSIS-DSP, CMSIS-RTOS API and CMSIS-SVD remain unchanged
    </release>
    <release version="3.20.0">
      The software portions that are deployed in the application program are now under a BSD license which allows usage
      of CMSIS components in any commercial or open source projects.  The Pack Description file Arm.CMSIS.pdsc describes the use cases
      The individual components have been update as listed below:
      - CMSIS-CORE adds functions for setting breakpoints, supports the latest GCC Compiler, and contains several corrections.
      - CMSIS-DSP library is optimized for more performance and contains several bug fixes.
      - CMSIS-RTOS API is extended with capabilities for short timeouts, Kernel initialization, and prepared for a C++ interface.
      - CMSIS-SVD is unchanged.
    </release>
  </releases>

  <taxonomy>
    <description Cclass="Board Support">Generic Interfaces for Evaluation and Development Boards</description>
    <description Cclass="CMSIS" doc="CMSIS/Documentation/General/html/index.html">Cortex Microcontroller Software Interface Components</description>
    <description Cclass="Device" doc="CMSIS/Documentation/Core/html/index.html">Startup, System Setup</description>
    <description Cclass="CMSIS Driver" doc="CMSIS/Documentation/Driver/html/index.html">Unified Device Drivers compliant to CMSIS-Driver Specifications</description>
    <description Cclass="File System">File Drive Support and File System</description>
    <description Cclass="Graphics">Graphical User Interface</description>
    <description Cclass="Network">Network Stack using Internet Protocols</description>
    <description Cclass="USB">Universal Serial Bus Stack</description>
    <description Cclass="Compiler">Compiler Software Extensions</description>
    <description Cclass="RTOS">Real-time Operating System</description>
  </taxonomy>

  <devices>
    <!-- ******************************  Cortex-M0  ****************************** -->
    <family Dfamily="ARM Cortex M0" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0497a/index.html" title="Cortex-M0 Device Generic Users Guide"/>
      <description>
The Cortex-M0 processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM0.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM0">
        <processor Dcore="Cortex-M0" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="NO_MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM0/Include/ARMCM0.h" define="ARMCM0"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M0P  ****************************** -->
    <family Dfamily="ARM Cortex M0 plus" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0662b/index.html" title="Cortex-M0+ Device Generic Users Guide"/>
      <description>
The Cortex-M0+ processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM0P.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM0P">
        <processor Dcore="Cortex-M0+" DcoreVersion="r0p1" Dfpu="NO_FPU" Dmpu="NO_MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM0plus/Include/ARMCM0plus.h" define="ARMCM0P"/>
      </device>

      <device Dname="ARMCM0P_MPU">
        <processor Dcore="Cortex-M0+" DcoreVersion="r0p1" Dfpu="NO_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM0plus/Include/ARMCM0plus_MPU.h" define="ARMCM0P_MPU"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M1  ****************************** -->
    <family Dfamily="ARM Cortex M1" Dvendor="ARM:82">
      <!--book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0497a/index.html" title="Cortex-M1 Device Generic Users Guide"/-->
      <description>
The ARM Cortex-M1 FPGA processor is intended for deeply embedded applications that require a small processor integrated into an FPGA.
The ARM Cortex-M1 processor implements the ARMv6-M architecture profile.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM0.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM1">
        <processor Dcore="Cortex-M1" DcoreVersion="r1p0" Dfpu="NO_FPU" Dmpu="NO_MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM1/Include/ARMCM1.h" define="ARMCM1"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M3  ****************************** -->
    <family Dfamily="ARM Cortex M3" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0552a/index.html" title="Cortex-M3 Device Generic Users Guide"/>
      <description>
The Cortex-M3 processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM3.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM3">
        <processor Dcore="Cortex-M3" DcoreVersion="r2p1" Dfpu="NO_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM3/Include/ARMCM3.h" define="ARMCM3"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M4  ****************************** -->
    <family Dfamily="ARM Cortex M4" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0553a/index.html" title="Cortex-M4 Device Generic Users Guide"/>
      <description>
The Cortex-M4 processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM4.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM4">
        <processor Dcore="Cortex-M4" DcoreVersion="r0p1" Dfpu="NO_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM4/Include/ARMCM4.h"    define="ARMCM4"/>
      </device>

      <device Dname="ARMCM4_FP">
        <processor Dcore="Cortex-M4" DcoreVersion="r0p1" Dfpu="SP_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM4/Include/ARMCM4_FP.h" define="ARMCM4_FP"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M7  ****************************** -->
    <family Dfamily="ARM Cortex M7" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.dui0646b/index.html" title="Cortex-M7 Device Generic Users Guide"/>
      <description>
The Cortex-M7 processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM7.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM7">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM7/Include/ARMCM7.h" define="ARMCM7"/>
      </device>

      <device Dname="ARMCM7_SP">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="SP_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM7/Include/ARMCM7_SP.h" define="ARMCM7_SP"/>
      </device>

      <device Dname="ARMCM7_DP">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="DP_FPU" Dmpu="MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM7/Include/ARMCM7_DP.h" define="ARMCM7_DP"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M23  ********************** -->
    <family Dfamily="ARM Cortex M23" Dvendor="ARM:82">
      <!--book name="Device/ARM/Documents/??_dgug.pdf"       title="?? Device Generic Users Guide"/-->
      <description>
The Arm Cortex-M23 is based on the Armv8-M baseline architecture.
It is the smallest and most energy efficient Arm processor with Arm TrustZone technology.
Cortex-M23 is the ideal processor for constrained embedded applications requiring efficient security.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM23.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IROM2"                                start="0x00200000" size="0x00200000" startup="0" default="0"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <memory id="IRAM2"                                start="0x20200000" size="0x00020000" init   ="0" default="0"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMCM23">
        <processor Dcore="Cortex-M23" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Dtz="NO_TZ" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM23/Include/ARMCM23.h" define="ARMCM23"/>
      </device>

      <device Dname="ARMCM23_TZ">
        <processor Dcore="Cortex-M23" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMCM23/Include/ARMCM23_TZ.h" define="ARMCM23_TZ"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M33  ****************************** -->
    <family Dfamily="ARM Cortex M33" Dvendor="ARM:82">
      <!--book name="Device/ARM/Documents/??_dgug.pdf"       title="?? Device Generic Users Guide"/-->
      <description>
The Arm Cortex-M33 is the most configurable of all Cortex-M processors. It is a full featured microcontroller
class processor based on the Armv8-M mainline architecture with Arm TrustZone security.
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMCM33.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IROM2"                                start="0x00200000" size="0x00200000" startup="0" default="0"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <memory id="IRAM2"                                start="0x20200000" size="0x00020000" init   ="0" default="0"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"          default="1"/-->

      <device Dname="ARMCM33">
        <processor Dcore="Cortex-M33" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Ddsp="NO_DSP" Dtz="NO_TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          no DSP Instructions, no Floating Point Unit, no TrustZone
        </description>
        <compile header="Device/ARM/ARMCM33/Include/ARMCM33.h" define="ARMCM33"/>
      </device>

      <device Dname="ARMCM33_TZ">
        <processor Dcore="Cortex-M33" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Ddsp="NO_DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          no DSP Instructions, no Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMCM33/Include/ARMCM33_TZ.h" define="ARMCM33_TZ"/>
      </device>

      <device Dname="ARMCM33_DSP_FP">
        <processor Dcore="Cortex-M33" DcoreVersion="r0p0" Dfpu="SP_FPU" Dmpu="MPU" Ddsp="DSP" Dtz="NO_TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          DSP Instructions, Single Precision Floating Point Unit, no TrustZone
        </description>
        <compile header="Device/ARM/ARMCM33/Include/ARMCM33_DSP_FP.h" define="ARMCM33_DSP_FP"/>
      </device>

      <device Dname="ARMCM33_DSP_FP_TZ">
        <processor Dcore="Cortex-M33" DcoreVersion="r0p0" Dfpu="SP_FPU" Dmpu="MPU" Ddsp="DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          DSP Instructions, Single Precision Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMCM33/Include/ARMCM33_DSP_FP_TZ.h" define="ARMCM33_DSP_FP_TZ"/>
      </device>
    </family>

    <!-- ******************************  ARMSC000  ****************************** -->
    <family Dfamily="ARM SC000" Dvendor="ARM:82">
      <description>
The Arm SC000 processor is an entry-level 32-bit Arm Cortex processor designed for a broad range of secure embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMSC000.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMSC000">
        <processor Dcore="SC000" DcoreVersion="r0p1" Dfpu="NO_FPU" Dmpu="NO_MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMSC000/Include/ARMSC000.h" define="ARMSC000"/>
      </device>
    </family>

    <!-- ******************************  ARMSC300  ****************************** -->
    <family Dfamily="ARM SC300" Dvendor="ARM:82">
      <description>
The ARM SC300 processor is an entry-level 32-bit ARM Cortex processor designed for a broad range of secure embedded applications. It offers significant benefits to developers, including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMSC300.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00040000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMSC300">
        <processor Dcore="SC300" DcoreVersion="r0p1" Dfpu="NO_FPU" Dmpu="NO_MPU" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMSC300/Include/ARMSC300.h" define="ARMSC300"/>
      </device>
    </family>

    <!-- ******************************  ARMv8-M Baseline  ********************** -->
    <family Dfamily="ARMv8-M Baseline" Dvendor="ARM:82">
      <!--book name="Device/ARM/Documents/ARMv8MBL_dgug.pdf"       title="ARMv8MBL Device Generic Users Guide"/-->
      <description>
Armv8-M Baseline based device with TrustZone
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMv8MBL.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IROM2"                                start="0x00200000" size="0x00200000" startup="0" default="0"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <memory id="IRAM2"                                start="0x20200000" size="0x00020000" init   ="0" default="0"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMv8MBL">
        <processor Dcore="ARMV8MBL" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <compile header="Device/ARM/ARMv8MBL/Include/ARMv8MBL.h" define="ARMv8MBL"/>
      </device>
    </family>

    <!-- ******************************  ARMv8-M Mainline  ****************************** -->
    <family Dfamily="ARMv8-M Mainline" Dvendor="ARM:82">
      <!--book name="Device/ARM/Documents/ARMv8MML_dgug.pdf"       title="ARMv8MML Device Generic Users Guide"/-->
      <description>
Armv8-M Mainline based device with TrustZone
      </description>
      <!-- debug svd="Device/ARM/SVD/ARMv8MML.svd"/ SVD files do not contain any peripheral -->
      <memory id="IROM1"                                start="0x00000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IROM2"                                start="0x00200000" size="0x00200000" startup="0" default="0"/>
      <memory id="IRAM1"                                start="0x20000000" size="0x00020000" init   ="0" default="1"/>
      <memory id="IRAM2"                                start="0x20200000" size="0x00020000" init   ="0" default="0"/>
      <!--algorithm name="Device/ARM/Flash/NEW_DEVICE.FLM" start="0x00000000" size="0x00040000"             default="1"/-->

      <device Dname="ARMv8MML">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Ddsp="NO_DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          no DSP Instructions, no Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML.h" define="ARMv8MML"/>
      </device>

      <device Dname="ARMv8MML_DSP">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p0" Dfpu="NO_FPU" Dmpu="MPU" Ddsp="DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          DSP Instructions, no Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML_DSP.h" define="ARMv8MML_DSP"/>
      </device>

      <device Dname="ARMv8MML_SP">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p1" Dfpu="SP_FPU" Dmpu="MPU" Ddsp="NO_DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          no DSP Instructions, Single Precision Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML_SP.h" define="ARMv8MML_SP"/>
      </device>

      <device Dname="ARMv8MML_DSP_SP">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p1" Dfpu="SP_FPU" Dmpu="MPU" Ddsp="DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          DSP Instructions, Single Precision Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML_DSP_SP.h" define="ARMv8MML_DSP_SP"/>
      </device>

      <device Dname="ARMv8MML_DP">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p1" Dfpu="DP_FPU" Dmpu="MPU" Ddsp="NO_DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          no DSP Instructions, Double Precision Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML_DP.h" define="ARMv8MML_DP"/>
      </device>

      <device Dname="ARMv8MML_DSP_DP">
        <processor Dcore="ARMV8MML" DcoreVersion="r0p1" Dfpu="DP_FPU" Dmpu="MPU" Ddsp="DSP" Dtz="TZ" Dendian="Configurable" Dclock="10000000"/>
        <description>
          DSP Instructions, Double Precision Floating Point Unit, TrustZone
        </description>
        <compile header="Device/ARM/ARMv8MML/Include/ARMv8MML_DSP_DP.h" define="ARMv8MML_DSP_DP"/>
      </device>
    </family>

    <!-- ******************************  Cortex-A5  ****************************** -->
    <family Dfamily="ARM Cortex A5" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.ddi0433c/index.html" title="Cortex-A5 Technical Reference Manual"/>
      <description>
The Arm Cortex-A5 processor is a high-performance, low-power, Arm macrocell with an L1 cache subsystem that provides full
virtual memory capabilities. The Cortex-A5 processor implements the Armv7-A architecture profile and can execute 32-bit
Arm instructions and 16-bit and 32-bit Thumb instructions. The Cortex-A5 is the smallest member of the Cortex-A processor family.
      </description>

      <memory id="IROM1"                                start="0x80000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x80200000" size="0x00200000" init   ="0" default="1"/>

      <device Dname="ARMCA5">
        <processor Dcore="Cortex-A5" DcoreVersion="r0p1" Dfpu="DP_FPU" Dmpu="MPU" Dendian="Configurable"/>
        <compile header="Device/ARM/ARMCA5/Include/ARMCA5.h" define="ARMCA5"/>
      </device>
    </family>

    <!-- ******************************  Cortex-A7  ****************************** -->
    <family Dfamily="ARM Cortex A7" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.ddi0464f/index.html" title="Cortex-A7 MPCore Technical Reference Manual"/>
      <description>
The Cortex-A7 MPCore processor is a high-performance, low-power processor that implements the Armv7-A architecture.
The Cortex-A7 MPCore processor has one to four processors in a single multiprocessor device with a L1 cache subsystem,
an optional integrated GIC, and an optional L2 cache controller.
      </description>

      <memory id="IROM1"                                start="0x80000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x80200000" size="0x00200000" init   ="0" default="1"/>

      <device Dname="ARMCA7">
        <processor Dcore="Cortex-A7" DcoreVersion="r0p5" Dfpu="DP_FPU" Dmpu="MPU" Dendian="Configurable"/>
        <compile header="Device/ARM/ARMCA7/Include/ARMCA7.h" define="ARMCA7"/>
      </device>
    </family>

    <!-- ******************************  Cortex-A9  ****************************** -->
    <family Dfamily="ARM Cortex A9" Dvendor="ARM:82">
      <book name="http://infocenter.arm.com/help/topic/com.arm.doc.100511_0401_10_en/index.html" title="Cortex-A9 Technical Reference Manual"/>
      <description>
The Cortex-A9 processor is a high-performance, low-power, Arm macrocell with an L1 cache subsystem that provides full virtual memory capabilities.
The Cortex-A9 processor implements the Armv7-A architecture and runs 32-bit Arm instructions, 16-bit and 32-bit Thumb instructions,
and 8-bit Java bytecodes in Jazelle state.
      </description>

      <memory id="IROM1"                                start="0x80000000" size="0x00200000" startup="1" default="1"/>
      <memory id="IRAM1"                                start="0x80200000" size="0x00200000" init   ="0" default="1"/>

      <device Dname="ARMCA9">
        <processor Dcore="Cortex-A9" DcoreVersion="r4p1" Dfpu="DP_FPU" Dmpu="MPU" Dendian="Configurable"/>
        <compile header="Device/ARM/ARMCA9/Include/ARMCA9.h" define="ARMCA9"/>
      </device>
    </family>
  </devices>


  <apis>
    <!-- CMSIS Device API -->
    <api Cclass="Device" Cgroup="IRQ Controller" Capiversion="1.0.0" exclusive="1">
      <description>Device interrupt controller interface</description>
      <files>
        <file category="header" name="CMSIS/Core_A/Include/irq_ctrl.h"/>
      </files>
    </api>
    <api Cclass="Device" Cgroup="OS Tick" Capiversion="1.0.1" exclusive="1">
      <description>RTOS Kernel system tick timer interface</description>
      <files>
        <file category="header" name="CMSIS/RTOS2/Include/os_tick.h"/>
      </files>
    </api>
    <!-- CMSIS-RTOS API -->
    <api Cclass="CMSIS" Cgroup="RTOS" Capiversion="1.0.0" exclusive="1">
      <description>CMSIS-RTOS API for Cortex-M, SC000, and SC300</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/RTOS/html/index.html"/>
      </files>
    </api>
    <api Cclass="CMSIS" Cgroup="RTOS2" Capiversion="2.1.3" exclusive="1">
      <description>CMSIS-RTOS API for Cortex-M, SC000, and SC300</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/RTOS2/html/index.html"/>
        <file category="header" name="CMSIS/RTOS2/Include/cmsis_os2.h"/>
      </files>
    </api>
    <!-- CMSIS Driver API -->
    <api Cclass="CMSIS Driver" Cgroup="USART" Capiversion="2.3.0" exclusive="0">
      <description>USART Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__usart__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_USART.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="SPI" Capiversion="2.2.0" exclusive="0">
      <description>SPI Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__spi__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_SPI.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="SAI" Capiversion="1.1.0" exclusive="0">
      <description>SAI Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__sai__interface__gr.html"/>
        <file category="header" name="CMSIS/Driver/Include/Driver_SAI.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="I2C" Capiversion="2.3.0" exclusive="0">
      <description>I2C Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__i2c__interface__gr.html"/>
        <file category="header" name="CMSIS/Driver/Include/Driver_I2C.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="CAN" Capiversion="1.2.0" exclusive="0">
      <description>CAN Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__can__interface__gr.html"/>
        <file category="header" name="CMSIS/Driver/Include/Driver_CAN.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="Flash" Capiversion="2.2.0" exclusive="0">
      <description>Flash Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__flash__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_Flash.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="MCI" Capiversion="2.3.0" exclusive="0">
      <description>MCI Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__mci__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_MCI.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="NAND" Capiversion="2.3.0" exclusive="0">
      <description>NAND Flash Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__nand__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_NAND.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet" Capiversion="2.1.0" exclusive="0">
      <description>Ethernet MAC and PHY Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__eth__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_ETH_MAC.h" />
        <file category="header" name="CMSIS/Driver/Include/Driver_ETH_PHY.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet MAC" Capiversion="2.1.0" exclusive="0">
      <description>Ethernet MAC Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__eth__mac__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_ETH_MAC.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet PHY" Capiversion="2.1.0" exclusive="0">
      <description>Ethernet PHY Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__eth__phy__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_ETH_PHY.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="USB Device" Capiversion="2.2.0" exclusive="0">
      <description>USB Device Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__usbd__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_USBD.h" />
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="USB Host" Capiversion="2.2.0" exclusive="0">
      <description>USB Host Driver API for Cortex-M</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/Driver/html/group__usbh__interface__gr.html" />
        <file category="header" name="CMSIS/Driver/Include/Driver_USBH.h" />
      </files>
    </api>
  </apis>

  <!-- conditions are dependency rules that can apply to a component or an individual file -->
  <conditions>
    <!-- compiler -->
    <condition id="ARMCC6">
      <accept Tcompiler="ARMCC" Toptions="AC6"/>
      <accept Tcompiler="ARMCC" Toptions="AC6LTO"/>
    </condition>
    <condition id="ARMCC5">
      <require Tcompiler="ARMCC" Toptions="AC5"/>
    </condition>
    <condition id="ARMCC">
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="GCC">
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="IAR">
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMCC GCC">
      <accept Tcompiler="ARMCC"/>
      <accept Tcompiler="GCC"/>
    </condition>
    <condition id="ARMCC GCC IAR">
      <accept Tcompiler="ARMCC"/>
      <accept Tcompiler="GCC"/>
      <accept Tcompiler="IAR"/>
    </condition>

    <!-- Arm architecture -->
    <condition id="ARMv6-M Device">
      <description>Armv6-M architecture based device</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M1"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
    </condition>
    <condition id="ARMv7-M Device">
      <description>Armv7-M architecture based device</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="Cortex-M4"/>
      <accept Dcore="Cortex-M7"/>
      <accept Dcore="SC300"/>
    </condition>
    <condition id="ARMv8-M Device">
      <description>Armv8-M architecture based device</description>
      <accept Dcore="ARMV8MBL"/>
      <accept Dcore="ARMV8MML"/>
      <accept Dcore="Cortex-M23"/>
      <accept Dcore="Cortex-M33"/>
    </condition>
    <condition id="ARMv8-M TZ Device">
      <description>Armv8-M architecture based device with TrustZone</description>
      <require condition="ARMv8-M Device"/>
      <require Dtz="TZ"/>
    </condition>
    <condition id="ARMv6_7-M Device">
      <description>Armv6_7-M architecture based device</description>
      <accept condition="ARMv6-M Device"/>
      <accept condition="ARMv7-M Device"/>
    </condition>
    <condition id="ARMv6_7_8-M Device">
      <description>Armv6_7_8-M architecture based device</description>
      <accept condition="ARMv6-M Device"/>
      <accept condition="ARMv7-M Device"/>
      <accept condition="ARMv8-M Device"/>
    </condition>
    <condition id="ARMv7-A Device">
      <description>Armv7-A architecture based device</description>
      <accept Dcore="Cortex-A5"/>
      <accept Dcore="Cortex-A7"/>
      <accept Dcore="Cortex-A9"/>
    </condition>

    <!-- ARM core -->
    <condition id="CM0">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
    </condition>
    <condition id="CM1">
      <description>Cortex-M1</description>
      <require Dcore="Cortex-M1"/>
    </condition>
    <condition id="CM3">
      <description>Cortex-M3 or SC300 processor based device</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
    </condition>
    <condition id="CM4">
      <description>Cortex-M4 processor based device</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU"/>
    </condition>
    <condition id="CM4_FP">
      <description>Cortex-M4 processor based device using Floating Point Unit</description>
      <accept Dcore="Cortex-M4" Dfpu="FPU"/>
      <accept Dcore="Cortex-M4" Dfpu="SP_FPU"/>
      <accept Dcore="Cortex-M4" Dfpu="DP_FPU"/>
    </condition>
    <condition id="CM7">
      <description>Cortex-M7 processor based device</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU"/>
    </condition>
    <condition id="CM7_FP">
      <description>Cortex-M7 processor based device using Floating Point Unit</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU"/>
    </condition>
    <condition id="CM7_SP">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP)</description>
      <require Dcore="Cortex-M7" Dfpu="SP_FPU"/>
    </condition>
    <condition id="CM7_DP">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP)</description>
      <require Dcore="Cortex-M7" Dfpu="DP_FPU"/>
    </condition>
    <condition id="CM23">
      <description>Cortex-M23 processor based device</description>
      <require Dcore="Cortex-M23"/>
    </condition>
    <condition id="CM33">
      <description>Cortex-M33 processor based device</description>
      <require Dcore="Cortex-M33" Dfpu="NO_FPU"/>
    </condition>
    <condition id="CM33_FP">
      <description>Cortex-M33 processor based device using Floating Point Unit</description>
      <require Dcore="Cortex-M33" Dfpu="SP_FPU"/>
    </condition>
    <condition id="ARMv8MBL">
      <description>Armv8-M Baseline processor based device</description>
      <require Dcore="ARMV8MBL"/>
    </condition>
    <condition id="ARMv8MML">
      <description>Armv8-M Mainline processor based device</description>
      <require Dcore="ARMV8MML" Dfpu="NO_FPU"/>
    </condition>
    <condition id="ARMv8MML_FP">
      <description>Armv8-M Mainline processor based device using Floating Point Unit</description>
      <accept Dcore="ARMV8MML" Dfpu="SP_FPU"/>
      <accept Dcore="ARMV8MML" Dfpu="DP_FPU"/>
    </condition>

    <condition id="CM33_NODSP_NOFPU">
      <description>CM33, no DSP, no FPU</description>
      <require Dcore="Cortex-M33" Ddsp="NO_DSP" Dfpu="NO_FPU"/>
    </condition>
    <condition id="CM33_DSP_NOFPU">
      <description>CM33, DSP, no FPU</description>
      <require Dcore="Cortex-M33" Ddsp="DSP" Dfpu="NO_FPU"/>
    </condition>
    <condition id="CM33_NODSP_SP">
      <description>CM33, no DSP, SP FPU</description>
      <require Dcore="Cortex-M33" Ddsp="NO_DSP" Dfpu="SP_FPU"/>
    </condition>
    <condition id="CM33_DSP_SP">
      <description>CM33, DSP, SP FPU</description>
      <require Dcore="Cortex-M33" Ddsp="DSP" Dfpu="SP_FPU"/>
    </condition>

    <condition id="ARMv8MML_NODSP_NOFPU">
      <description>Armv8-M Mainline, no DSP, no FPU</description>
      <require Dcore="ARMV8MML" Ddsp="NO_DSP" Dfpu="NO_FPU"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU">
      <description>Armv8-M Mainline, DSP, no FPU</description>
      <require Dcore="ARMV8MML" Ddsp="DSP" Dfpu="NO_FPU"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP">
      <description>Armv8-M Mainline, no DSP, SP FPU</description>
      <require Dcore="ARMV8MML" Ddsp="NO_DSP" Dfpu="SP_FPU"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP">
      <description>Armv8-M Mainline, DSP, SP FPU</description>
      <require Dcore="ARMV8MML" Ddsp="DSP" Dfpu="SP_FPU"/>
    </condition>

    <condition id="CA5_CA9">
      <description>Cortex-A5 or Cortex-A9 processor based device</description>
      <accept Dcore="Cortex-A5"/>
      <accept Dcore="Cortex-A9"/>
    </condition>

    <condition id="CA7">
      <description>Cortex-A7 processor based device</description>
      <accept Dcore="Cortex-A7"/>
    </condition>

    <!-- ARMCC compiler -->
    <condition id="CA_ARMCC5">
      <description>Cortex-A5, Cortex-A7 or Cortex-A9 processor based device for the Arm Compiler 5</description>
      <require condition="ARMv7-A Device"/>
      <require condition="ARMCC5"/>
    </condition>
    <condition id="CA_ARMCC6">
      <description>Cortex-A5, Cortex-A7 or Cortex-A9 processor based device for the Arm Compiler 6</description>
      <require condition="ARMv7-A Device"/>
      <require condition="ARMCC6"/>
    </condition>

    <condition id="CM0_ARMCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device for the Arm Compiler</description>
      <require condition="CM0"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM0_LE_ARMCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM0_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM0_BE_ARMCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM0_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM1_ARMCC">
      <description>Cortex-M1 based device for the Arm Compiler</description>
      <require condition="CM1"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM1_LE_ARMCC">
      <description>Cortex-M1 based device in little endian mode for the Arm Compiler</description>
      <require condition="CM1_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM1_BE_ARMCC">
      <description>Cortex-M1 based device in big endian mode for the Arm Compiler</description>
      <require condition="CM1_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM3_ARMCC">
      <description>Cortex-M3 or SC300 processor based device for the Arm Compiler</description>
      <require condition="CM3"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM3_LE_ARMCC">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM3_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM3_BE_ARMCC">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM3_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_ARMCC">
      <description>Cortex-M4 processor based device for the Arm Compiler</description>
      <require condition="CM4"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM4_LE_ARMCC">
      <description>Cortex-M4 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM4_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_BE_ARMCC">
      <description>Cortex-M4 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM4_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_FP_ARMCC">
      <description>Cortex-M4 processor based device using Floating Point Unit for the Arm Compiler</description>
      <require condition="CM4_FP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM4_FP_LE_ARMCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the Arm Compiler</description>
      <require condition="CM4_FP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_FP_BE_ARMCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the Arm Compiler</description>
      <require condition="CM4_FP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_ARMCC">
      <description>Cortex-M7 processor based device for the Arm Compiler</description>
      <require condition="CM7"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM7_LE_ARMCC">
      <description>Cortex-M7 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM7_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_BE_ARMCC">
      <description>Cortex-M7 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM7_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_FP_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit for the Arm Compiler</description>
      <require condition="CM7_FP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM7_FP_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the Arm Compiler</description>
      <require condition="CM7_FP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_FP_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the Arm Compiler</description>
      <require condition="CM7_FP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_SP_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) for the Arm Compiler</description>
      <require condition="CM7_SP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM7_SP_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in little endian mode for the Arm Compiler</description>
      <require condition="CM7_SP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_SP_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in big endian mode for the Arm Compiler</description>
      <require condition="CM7_SP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_DP_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) for the Arm Compiler</description>
      <require condition="CM7_DP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM7_DP_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in little endian mode for the Arm Compiler</description>
      <require condition="CM7_DP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_DP_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in big endian mode for the Arm Compiler</description>
      <require condition="CM7_DP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM23_ARMCC">
      <description>Cortex-M23 processor based device for the Arm Compiler</description>
      <require condition="CM23"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM23_LE_ARMCC">
      <description>Cortex-M23 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM23_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM23_BE_ARMCC">
      <description>Cortex-M23 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM23_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_ARMCC">
      <description>Cortex-M33 processor based device for the Arm Compiler</description>
      <require condition="CM33"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_LE_ARMCC">
      <description>Cortex-M33 processor based device in little endian mode for the Arm Compiler</description>
      <require condition="CM33_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_BE_ARMCC">
      <description>Cortex-M33 processor based device in big endian mode for the Arm Compiler</description>
      <require condition="CM33_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_FP_ARMCC">
      <description>Cortex-M33 processor based device using Floating Point Unit for the Arm Compiler</description>
      <require condition="CM33_FP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_FP_LE_ARMCC">
      <description>Cortex-M33 processor based device using Floating Point Unit in little endian mode for the Arm Compiler</description>
      <require condition="CM33_FP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_FP_BE_ARMCC">
      <description>Cortex-M33 processor based device using Floating Point Unit in big endian mode for the Arm Compiler</description>
      <require condition="CM33_FP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_NODSP_NOFPU_ARMCC">
      <description>Cortex-M33 processor, no DSP, no FPU, Arm Compiler</description>
      <require condition="CM33_NODSP_NOFPU"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_ARMCC">
      <description>Cortex-M33 processor, DSP, no FPU, Arm Compiler</description>
      <require condition="CM33_DSP_NOFPU"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_NODSP_SP_ARMCC">
      <description>Cortex-M33 processor, no DSP, SP FPU, Arm Compiler</description>
      <require condition="CM33_NODSP_SP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_DSP_SP_ARMCC">
      <description>Cortex-M33 processor, DSP, SP FPU, Arm Compiler</description>
      <require condition="CM33_DSP_SP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM33_NODSP_NOFPU_LE_ARMCC">
      <description>Cortex-M33 processor, little endian, no DSP, no FPU, Arm Compiler</description>
      <require condition="CM33_NODSP_NOFPU_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_LE_ARMCC">
      <description>Cortex-M33 processor, little endian, DSP, no FPU, Arm Compiler</description>
      <require condition="CM33_DSP_NOFPU_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_NODSP_SP_LE_ARMCC">
      <description>Cortex-M33 processor, little endian, no DSP, SP FPU, Arm Compiler</description>
      <require condition="CM33_NODSP_SP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_SP_LE_ARMCC">
      <description>Cortex-M33 processor, little endian, DSP, SP FPU, Arm Compiler</description>
      <require condition="CM33_DSP_SP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>

    <condition id="ARMv8MBL_ARMCC">
      <description>Armv8-M Baseline processor based device for the Arm Compiler</description>
      <require condition="ARMv8MBL"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MBL_LE_ARMCC">
      <description>Armv8-M Baseline processor based device in little endian mode for the Arm Compiler</description>
      <require condition="ARMv8MBL_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MBL_BE_ARMCC">
      <description>Armv8-M Baseline processor based device in big endian mode for the Arm Compiler</description>
      <require condition="ARMv8MBL_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_ARMCC">
      <description>Armv8-M Mainline processor based device for the Arm Compiler</description>
      <require condition="ARMv8MML"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_LE_ARMCC">
      <description>Armv8-M Mainline processor based device in little endian mode for the Arm Compiler</description>
      <require condition="ARMv8MML_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_BE_ARMCC">
      <description>Armv8-M Mainline processor based device in big endian mode for the Arm Compiler</description>
      <require condition="ARMv8MML_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_FP_ARMCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit for the Arm Compiler</description>
      <require condition="ARMv8MML_FP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_FP_LE_ARMCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in little endian mode for the Arm Compiler</description>
      <require condition="ARMv8MML_FP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_FP_BE_ARMCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in big endian mode for the Arm Compiler</description>
      <require condition="ARMv8MML_FP_ARMCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_NODSP_NOFPU_ARMCC">
      <description>Armv8-M Mainline, no DSP, no FPU, Arm Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_ARMCC">
      <description>Armv8-M Mainline, DSP, no FPU, Arm Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_ARMCC">
      <description>Armv8-M Mainline, no DSP, SP FPU, Arm Compiler</description>
      <require condition="ARMv8MML_NODSP_SP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_ARMCC">
      <description>Armv8-M Mainline, DSP, SP FPU, Arm Compiler</description>
      <require condition="ARMv8MML_DSP_SP"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="ARMv8MML_NODSP_NOFPU_LE_ARMCC">
      <description>Armv8-M Mainline, little endian, no DSP, no FPU, Arm Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_LE_ARMCC">
      <description>Armv8-M Mainline, little endian, DSP, no FPU, Arm Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_LE_ARMCC">
      <description>Armv8-M Mainline, little endian, no DSP, SP FPU, Arm Compiler</description>
      <require condition="ARMv8MML_NODSP_SP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_LE_ARMCC">
      <description>Armv8-M Mainline, little endian, DSP, SP FPU, Arm Compiler</description>
      <require condition="ARMv8MML_DSP_SP_ARMCC"/>
      <require Dendian="Little-endian"/>
    </condition>

    <!-- GCC compiler -->
    <condition id="CA_GCC">
      <description>Cortex-A5, Cortex-A7 or Cortex-A9 processor based device for the GCC Compiler</description>
      <require condition="ARMv7-A Device"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM0_GCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device for the GCC Compiler</description>
      <require condition="CM0"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM0_LE_GCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM0_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM0_BE_GCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM0_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM1_GCC">
      <description>Cortex-M1 based device for the GCC Compiler</description>
      <require condition="CM1"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM1_LE_GCC">
      <description>Cortex-M1 based device in little endian mode for the GCC Compiler</description>
      <require condition="CM1_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM1_BE_GCC">
      <description>Cortex-M1 based device in big endian mode for the GCC Compiler</description>
      <require condition="CM1_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM3_GCC">
      <description>Cortex-M3 or SC300 processor based device for the GCC Compiler</description>
      <require condition="CM3"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM3_LE_GCC">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM3_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM3_BE_GCC">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM3_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_GCC">
      <description>Cortex-M4 processor based device for the GCC Compiler</description>
      <require condition="CM4"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM4_LE_GCC">
      <description>Cortex-M4 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM4_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_BE_GCC">
      <description>Cortex-M4 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM4_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_FP_GCC">
      <description>Cortex-M4 processor based device using Floating Point Unit for the GCC Compiler</description>
      <require condition="CM4_FP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM4_FP_LE_GCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <require condition="CM4_FP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_FP_BE_GCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <require condition="CM4_FP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_GCC">
      <description>Cortex-M7 processor based device for the GCC Compiler</description>
      <require condition="CM7"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM7_LE_GCC">
      <description>Cortex-M7 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM7_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_BE_GCC">
      <description>Cortex-M7 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM7_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_FP_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit for the GCC Compiler</description>
      <require condition="CM7_FP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM7_FP_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <require condition="CM7_FP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_FP_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <require condition="CM7_FP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_SP_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) for the GCC Compiler</description>
      <require condition="CM7_SP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM7_SP_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in little endian mode for the GCC Compiler</description>
      <require condition="CM7_SP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_SP_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in big endian mode for the GCC Compiler</description>
      <require condition="CM7_SP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_DP_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) for the GCC Compiler</description>
      <require condition="CM7_DP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM7_DP_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in little endian mode for the GCC Compiler</description>
      <require condition="CM7_DP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_DP_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in big endian mode for the GCC Compiler</description>
      <require condition="CM7_DP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM23_GCC">
      <description>Cortex-M23 processor based device for the GCC Compiler</description>
      <require condition="CM23"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM23_LE_GCC">
      <description>Cortex-M23 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM23_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM23_BE_GCC">
      <description>Cortex-M23 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM23_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_GCC">
      <description>Cortex-M33 processor based device for the GCC Compiler</description>
      <require condition="CM33"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_LE_GCC">
      <description>Cortex-M33 processor based device in little endian mode for the GCC Compiler</description>
      <require condition="CM33_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_BE_GCC">
      <description>Cortex-M33 processor based device in big endian mode for the GCC Compiler</description>
      <require condition="CM33_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_FP_GCC">
      <description>Cortex-M33 processor based device using Floating Point Unit for the GCC Compiler</description>
      <require condition="CM33_FP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_FP_LE_GCC">
      <description>Cortex-M33 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <require condition="CM33_FP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_FP_BE_GCC">
      <description>Cortex-M33 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <require condition="CM33_FP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_NODSP_NOFPU_GCC">
      <description>CM33, no DSP, no FPU, GCC Compiler</description>
      <require condition="CM33_NODSP_NOFPU"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_GCC">
      <description>CM33, DSP, no FPU, GCC Compiler</description>
      <require condition="CM33_DSP_NOFPU"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_NODSP_SP_GCC">
      <description>CM33, no DSP, SP FPU, GCC Compiler</description>
      <require condition="CM33_NODSP_SP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_DSP_SP_GCC">
      <description>CM33, DSP, SP FPU, GCC Compiler</description>
      <require condition="CM33_DSP_SP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM33_NODSP_NOFPU_LE_GCC">
      <description>CM33, little endian, no DSP, no FPU, GCC Compiler</description>
      <require condition="CM33_NODSP_NOFPU_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_LE_GCC">
      <description>CM33, little endian, DSP, no FPU, GCC Compiler</description>
      <require condition="CM33_DSP_NOFPU_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_NODSP_SP_LE_GCC">
      <description>CM33, little endian, no DSP, SP FPU, GCC Compiler</description>
      <require condition="CM33_NODSP_SP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_SP_LE_GCC">
      <description>CM33, little endian, DSP, SP FPU, GCC Compiler</description>
      <require condition="CM33_DSP_SP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>

    <condition id="ARMv8MBL_GCC">
      <description>Armv8-M Baseline processor based device for the GCC Compiler</description>
      <require condition="ARMv8MBL"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MBL_LE_GCC">
      <description>Armv8-M Baseline processor based device in little endian mode for the GCC Compiler</description>
      <require condition="ARMv8MBL_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MBL_BE_GCC">
      <description>Armv8-M Baseline processor based device in big endian mode for the GCC Compiler</description>
      <require condition="ARMv8MBL_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_GCC">
      <description>Armv8-M Mainline processor based device for the GCC Compiler</description>
      <require condition="ARMv8MML"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_LE_GCC">
      <description>Armv8-M Mainline processor based device in little endian mode for the GCC Compiler</description>
      <require condition="ARMv8MML_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_BE_GCC">
      <description>Armv8-M Mainline processor based device in big endian mode for the GCC Compiler</description>
      <require condition="ARMv8MML_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_FP_GCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit for the GCC Compiler</description>
      <require condition="ARMv8MML_FP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_FP_LE_GCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <require condition="ARMv8MML_FP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_FP_BE_GCC">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <require condition="ARMv8MML_FP_GCC"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_NODSP_NOFPU_GCC">
      <description>Armv8-M Mainline, no DSP, no FPU, GCC Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_GCC">
      <description>Armv8-M Mainline, DSP, no FPU, GCC Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_GCC">
      <description>Armv8-M Mainline, no DSP, SP FPU, GCC Compiler</description>
      <require condition="ARMv8MML_NODSP_SP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_GCC">
      <description>Armv8-M Mainline, DSP, SP FPU, GCC Compiler</description>
      <require condition="ARMv8MML_DSP_SP"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="ARMv8MML_NODSP_NOFPU_LE_GCC">
      <description>Armv8-M Mainline, little endian, no DSP, no FPU, GCC Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_LE_GCC">
      <description>Armv8-M Mainline, little endian, DSP, no FPU, GCC Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_LE_GCC">
      <description>Armv8-M Mainline, little endian, no DSP, SP FPU, GCC Compiler</description>
      <require condition="ARMv8MML_NODSP_SP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_LE_GCC">
      <description>Armv8-M Mainline, little endian, DSP, SP FPU, GCC Compiler</description>
      <require condition="ARMv8MML_DSP_SP_GCC"/>
      <require Dendian="Little-endian"/>
    </condition>

    <!-- IAR compiler -->
    <condition id="CA_IAR">
      <description>Cortex-A5, Cortex-A7 or Cortex-A9 processor based device for the IAR Compiler</description>
      <require condition="ARMv7-A Device"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM0_IAR">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device for the IAR Compiler</description>
      <require condition="CM0"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM0_LE_IAR">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM0_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM0_BE_IAR">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM0_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM1_IAR">
      <description>Cortex-M1 based device for the IAR Compiler</description>
      <require condition="CM1"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM1_LE_IAR">
      <description>Cortex-M1 based device in little endian mode for the IAR Compiler</description>
      <require condition="CM1_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM1_BE_IAR">
      <description>Cortex-M1 based device in big endian mode for the IAR Compiler</description>
      <require condition="CM1_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM3_IAR">
      <description>Cortex-M3 or SC300 processor based device for the IAR Compiler</description>
      <require condition="CM3"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM3_LE_IAR">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM3_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM3_BE_IAR">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM3_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_IAR">
      <description>Cortex-M4 processor based device for the IAR Compiler</description>
      <require condition="CM4"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM4_LE_IAR">
      <description>Cortex-M4 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM4_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_BE_IAR">
      <description>Cortex-M4 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM4_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM4_FP_IAR">
      <description>Cortex-M4 processor based device using Floating Point Unit for the IAR Compiler</description>
      <require condition="CM4_FP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM4_FP_LE_IAR">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <require condition="CM4_FP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM4_FP_BE_IAR">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <require condition="CM4_FP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_IAR">
      <description>Cortex-M7 processor based device for the IAR Compiler</description>
      <require condition="CM7"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM7_LE_IAR">
      <description>Cortex-M7 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM7_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_BE_IAR">
      <description>Cortex-M7 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM7_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_FP_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit for the IAR Compiler</description>
      <require condition="CM7_FP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM7_FP_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <require condition="CM7_FP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_FP_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <require condition="CM7_FP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_SP_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) for the IAR Compiler</description>
      <require condition="CM7_SP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM7_SP_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in little endian mode for the IAR Compiler</description>
      <require condition="CM7_SP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_SP_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (SP) in big endian mode for the IAR Compiler</description>
      <require condition="CM7_SP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM7_DP_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) for the IAR Compiler</description>
      <require condition="CM7_DP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM7_DP_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in little endian mode for the IAR Compiler</description>
      <require condition="CM7_DP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM7_DP_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit (DP) in big endian mode for the IAR Compiler</description>
      <require condition="CM7_DP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM23_IAR">
      <description>Cortex-M23 processor based device for the IAR Compiler</description>
      <require condition="CM23"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM23_LE_IAR">
      <description>Cortex-M23 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM23_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM23_BE_IAR">
      <description>Cortex-M23 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM23_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_IAR">
      <description>Cortex-M33 processor based device for the IAR Compiler</description>
      <require condition="CM33"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_LE_IAR">
      <description>Cortex-M33 processor based device in little endian mode for the IAR Compiler</description>
      <require condition="CM33_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_BE_IAR">
      <description>Cortex-M33 processor based device in big endian mode for the IAR Compiler</description>
      <require condition="CM33_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_FP_IAR">
      <description>Cortex-M33 processor based device using Floating Point Unit for the IAR Compiler</description>
      <require condition="CM33_FP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_FP_LE_IAR">
      <description>Cortex-M33 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <require condition="CM33_FP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_FP_BE_IAR">
      <description>Cortex-M33 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <require condition="CM33_FP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="CM33_NODSP_NOFPU_IAR">
      <description>CM33, no DSP, no FPU, IAR Compiler</description>
      <require condition="CM33_NODSP_NOFPU"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_IAR">
      <description>CM33, DSP, no FPU, IAR Compiler</description>
      <require condition="CM33_DSP_NOFPU"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_NODSP_SP_IAR">
      <description>CM33, no DSP, SP FPU, IAR Compiler</description>
      <require condition="CM33_NODSP_SP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_DSP_SP_IAR">
      <description>CM33, DSP, SP FPU, IAR Compiler</description>
      <require condition="CM33_DSP_SP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="CM33_NODSP_NOFPU_LE_IAR">
      <description>CM33, little endian, no DSP, no FPU, IAR Compiler</description>
      <require condition="CM33_NODSP_NOFPU_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_NOFPU_LE_IAR">
      <description>CM33, little endian, DSP, no FPU, IAR Compiler</description>
      <require condition="CM33_DSP_NOFPU_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_NODSP_SP_LE_IAR">
      <description>CM33, little endian, no DSP, SP FPU, IAR Compiler</description>
      <require condition="CM33_NODSP_SP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="CM33_DSP_SP_LE_IAR">
      <description>CM33, little endian, DSP, SP FPU, IAR Compiler</description>
      <require condition="CM33_DSP_SP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>

    <condition id="ARMv8MBL_IAR">
      <description>Armv8-M Baseline processor based device for the IAR Compiler</description>
      <require condition="ARMv8MBL"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MBL_LE_IAR">
      <description>Armv8-M Baseline processor based device in little endian mode for the IAR Compiler</description>
      <require condition="ARMv8MBL_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MBL_BE_IAR">
      <description>Armv8-M Baseline processor based device in big endian mode for the IAR Compiler</description>
      <require condition="ARMv8MBL_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_IAR">
      <description>Armv8-M Mainline processor based device for the IAR Compiler</description>
      <require condition="ARMv8MML"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_LE_IAR">
      <description>Armv8-M Mainline processor based device in little endian mode for the IAR Compiler</description>
      <require condition="ARMv8MML_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_BE_IAR">
      <description>Armv8-M Mainline processor based device in big endian mode for the IAR Compiler</description>
      <require condition="ARMv8MML_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_FP_IAR">
      <description>Armv8-M Mainline processor based device using Floating Point Unit for the IAR Compiler</description>
      <require condition="ARMv8MML_FP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_FP_LE_IAR">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <require condition="ARMv8MML_FP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_FP_BE_IAR">
      <description>Armv8-M Mainline processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <require condition="ARMv8MML_FP_IAR"/>
      <require Dendian="Big-endian"/>
    </condition>

    <condition id="ARMv8MML_NODSP_NOFPU_IAR">
      <description>Armv8-M Mainline, no DSP, no FPU, IAR Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_IAR">
      <description>Armv8-M Mainline, DSP, no FPU, IAR Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_IAR">
      <description>Armv8-M Mainline, no DSP, SP FPU, IAR Compiler</description>
      <require condition="ARMv8MML_NODSP_SP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_IAR">
      <description>Armv8-M Mainline, DSP, SP FPU, IAR Compiler</description>
      <require condition="ARMv8MML_DSP_SP"/>
      <require Tcompiler="IAR"/>
    </condition>
    <condition id="ARMv8MML_NODSP_NOFPU_LE_IAR">
      <description>Armv8-M Mainline, little endian, no DSP, no FPU, IAR Compiler</description>
      <require condition="ARMv8MML_NODSP_NOFPU_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_NOFPU_LE_IAR">
      <description>Armv8-M Mainline, little endian, DSP, no FPU, IAR Compiler</description>
      <require condition="ARMv8MML_DSP_NOFPU_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_NODSP_SP_LE_IAR">
      <description>Armv8-M Mainline, little endian, no DSP, SP FPU, IAR Compiler</description>
      <require condition="ARMv8MML_NODSP_SP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>
    <condition id="ARMv8MML_DSP_SP_LE_IAR">
      <description>Armv8-M Mainline, little endian, DSP, SP FPU, IAR Compiler</description>
      <require condition="ARMv8MML_DSP_SP_IAR"/>
      <require Dendian="Little-endian"/>
    </condition>

    <!-- conditions selecting single devices and CMSIS Core -->
    <!-- used for component startup, GCC version is used for C-Startup -->
    <condition id="ARMCM0 CMSIS">
      <description>Generic Arm Cortex-M0 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM0"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM0 CMSIS GCC">
      <description>Generic ARM Cortex-M0 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM0 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM0+ CMSIS">
      <description>Generic Arm Cortex-M0+ device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM0P*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM0+ CMSIS GCC">
      <description>Generic Arm Cortex-M0+ device startup and depends CMSIS Core requiring GCC</description>
      <require condition="ARMCM0+ CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM1 CMSIS">
      <description>Generic Arm Cortex-M1 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM1"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM1 CMSIS GCC">
      <description>Generic ARM Cortex-M1 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM1 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM3 CMSIS">
      <description>Generic Arm Cortex-M3 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM3"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM3 CMSIS GCC">
      <description>Generic Arm Cortex-M3 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM3 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM4 CMSIS">
      <description>Generic Arm Cortex-M4 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM4*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM4 CMSIS GCC">
      <description>Generic Arm Cortex-M4 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM4 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM7 CMSIS">
      <description>Generic Arm Cortex-M7 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM7*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM7 CMSIS GCC">
      <description>Generic Arm Cortex-M7 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM7 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM23 CMSIS">
      <description>Generic Arm Cortex-M23 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM23*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM23 CMSIS GCC">
      <description>Generic Arm Cortex-M23 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM23 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM33 CMSIS">
      <description>Generic Arm Cortex-M33 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM33*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMCM33 CMSIS GCC">
      <description>Generic Arm Cortex-M33 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMCM33 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMSC000 CMSIS">
      <description>Generic Arm SC000 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMSC000"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMSC000 CMSIS GCC">
      <description>Generic Arm SC000 device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMSC000 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMSC300 CMSIS">
      <description>Generic Arm SC300 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMSC300"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMSC300 CMSIS GCC">
      <description>Generic Arm SC300 device startup and dependson CMSIS Core requiring GCC</description>
      <require condition="ARMSC300 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMv8MBL CMSIS">
      <description>Generic Armv8-M Baseline device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMv8MBL"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMv8MBL CMSIS GCC">
      <description>Generic Armv8-M Baseline device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMv8MBL CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMv8MML CMSIS">
      <description>Generic Armv8-M Mainline device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMv8MML*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>
    <condition id="ARMv8MML CMSIS GCC">
      <description>Generic Armv8-M Mainline device startup and depends on CMSIS Core requiring GCC</description>
      <require condition="ARMv8MML CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCA5 CMSIS">
      <description>Generic Arm Cortex-A5 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCA5"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCA7 CMSIS">
      <description>Generic Arm Cortex-A7 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCA7"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCA9 CMSIS">
      <description>Generic Arm Cortex-A9 device startup and depends on CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCA9"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <!-- CMSIS DSP -->
    <condition id="CMSIS DSP">
      <description>Components required for DSP</description>
      <require condition="ARMv6_7_8-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <!-- CMSIS NN -->
    <condition id="CMSIS NN">
      <description>Components required for NN</description>
      <require condition="CMSIS DSP"/>
    </condition>

    <!-- RTOS RTX -->
    <condition id="RTOS RTX">
      <description>Components required for RTOS RTX</description>
      <require condition="ARMv6_7-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="Device" Cgroup="Startup"/>
      <deny    Cclass="CMSIS"  Cgroup="RTOS2" Csub="Keil RTX5"/>
    </condition>
    <condition id="RTOS RTX IFX">
      <description>Components required for RTOS RTX IFX</description>
      <require condition="ARMv6_7-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Cclass="Device" Cgroup="Startup"/>
      <deny    Cclass="CMSIS"  Cgroup="RTOS2" Csub="Keil RTX5"/>
    </condition>
    <condition id="RTOS RTX5">
      <description>Components required for RTOS RTX5</description>
      <require condition="ARMv6_7_8-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS"  Cgroup="RTOS2" Csub="Keil RTX5"/>
    </condition>
    <condition id="RTOS2 RTX5">
      <description>Components required for RTOS2 RTX5</description>
      <require condition="ARMv6_7_8-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS"  Cgroup="CORE"/>
      <require Cclass="Device" Cgroup="Startup"/>
    </condition>
    <condition id="RTOS2 RTX5 v7-A">
      <description>Components required for RTOS2 RTX5 on Armv7-A</description>
      <require condition="ARMv7-A Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS"  Cgroup="CORE"/>
      <require Cclass="Device" Cgroup="Startup"/>
      <require Cclass="Device" Cgroup="OS Tick"/>
      <require Cclass="Device" Cgroup="IRQ Controller"/>
    </condition>
    <condition id="RTOS2 RTX5 Lib">
      <description>Components required for RTOS2 RTX5 Library</description>
      <require condition="ARMv6_7_8-M Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS"  Cgroup="CORE"/>
      <require Cclass="Device" Cgroup="Startup"/>
    </condition>
    <condition id="RTOS2 RTX5 NS">
      <description>Components required for RTOS2 RTX5 in Non-Secure Domain</description>
      <require condition="ARMv8-M TZ Device"/>
      <require condition="ARMCC GCC IAR"/>
      <require Cclass="CMSIS"  Cgroup="CORE"/>
      <require Cclass="Device" Cgroup="Startup"/>
    </condition>

    <!-- OS Tick -->
    <condition id="OS Tick PTIM">
      <description>Components required for OS Tick Private Timer</description>
      <require condition="CA5_CA9"/>
      <require Cclass="Device" Cgroup="IRQ Controller"/>
    </condition>

    <condition id="OS Tick GTIM">
      <description>Components required for OS Tick Generic Physical Timer</description>
      <require condition="CA7"/>
      <require Cclass="Device" Cgroup="IRQ Controller"/>
    </condition>

  </conditions>

  <components>
    <!-- CMSIS-Core component -->
    <component Cclass="CMSIS" Cgroup="CORE" Cversion="5.1.2"  condition="ARMv6_7_8-M Device" >
      <description>CMSIS-CORE for Cortex-M, SC000, SC300, ARMv8-M</description>
      <files>
        <!-- CPU independent -->
        <file category="doc"     name="CMSIS/Documentation/Core/html/index.html"/>
        <file category="include" name="CMSIS/Core/Include/"/>
        <file category="header"  name="CMSIS/Core/Include/tz_context.h" condition="ARMv8-M TZ Device"/>
        <!-- Code template -->
        <file category="sourceC" attr="template" condition="ARMv8-M TZ Device" name="CMSIS/Core/Template/ARMv8-M/main_s.c"     version="1.1.0" select="Secure mode 'main' module for ARMv8-M"/>
        <file category="sourceC" attr="template" condition="ARMv8-M TZ Device" name="CMSIS/Core/Template/ARMv8-M/tz_context.c" version="1.1.0" select="RTOS Context Management (TrustZone for ARMv8-M)" />
      </files>
    </component>

    <component Cclass="CMSIS" Cgroup="CORE" Cversion="1.1.2"  condition="ARMv7-A Device" >
      <description>CMSIS-CORE for Cortex-A</description>
      <files>
        <!-- CPU independent -->
        <file category="doc"     name="CMSIS/Documentation/Core_A/html/index.html"/>
        <file category="include" name="CMSIS/Core_A/Include/"/>
      </files>
    </component>

    <!-- CMSIS-Startup components -->
    <!-- Cortex-M0 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM0 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M0 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM0/Include/ARMCM0.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM0/Source/ARM/startup_ARMCM0.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM0/Source/GCC/startup_ARMCM0.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM0/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM0/Source/IAR/startup_ARMCM0.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM0/Source/system_ARMCM0.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM0 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M0 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM0/Include/ARMCM0.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM0/Source/GCC/startup_ARMCM0.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM0/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM0/Source/system_ARMCM0.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M0+ -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM0+ CMSIS">
      <description>System and Startup for Generic Arm Cortex-M0+ device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM0plus/Include/ARMCM0plus.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM0plus/Source/ARM/startup_ARMCM0plus.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM0plus/Source/GCC/startup_ARMCM0plus.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM0plus/Source/GCC/gcc_arm.ld"           version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM0plus/Source/IAR/startup_ARMCM0plus.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM0plus/Source/system_ARMCM0plus.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM0+ CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M0+ device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM0plus/Include/ARMCM0plus.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM0plus/Source/GCC/startup_ARMCM0plus.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM0plus/Source/GCC/gcc_arm.ld"           version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM0plus/Source/system_ARMCM0plus.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M1 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM1 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M1 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM1/Include/ARMCM1.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM1/Source/ARM/startup_ARMCM1.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM1/Source/GCC/startup_ARMCM1.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM1/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM1/Source/IAR/startup_ARMCM1.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM1/Source/system_ARMCM1.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM1 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M1 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM1/Include/ARMCM1.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM1/Source/GCC/startup_ARMCM1.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM1/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM1/Source/system_ARMCM1.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M3 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM3 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M3 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM3/Include/ARMCM3.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM3/Source/ARM/startup_ARMCM3.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM3/Source/GCC/startup_ARMCM3.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM3/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM3/Source/IAR/startup_ARMCM3.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM3/Source/system_ARMCM3.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM3 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M3 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMCM3/Include/ARMCM3.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM3/Source/GCC/startup_ARMCM3.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM3/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM3/Source/system_ARMCM3.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M4 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM4 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M4 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include" name="Device/ARM/ARMCM4/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM4/Source/ARM/startup_ARMCM4.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM4/Source/GCC/startup_ARMCM4.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM4/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM4/Source/IAR/startup_ARMCM4.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM4/Source/system_ARMCM4.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM4 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M4 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include" name="Device/ARM/ARMCM4/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM4/Source/GCC/startup_ARMCM4.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM4/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM4/Source/system_ARMCM4.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M7 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCM7 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M7 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMCM7/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM7/Source/ARM/startup_ARMCM7.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM7/Source/GCC/startup_ARMCM7.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM7/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM7/Source/IAR/startup_ARMCM7.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM7/Source/system_ARMCM7.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMCM7 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M7 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMCM7/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM7/Source/GCC/startup_ARMCM7.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM7/Source/GCC/gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM7/Source/system_ARMCM7.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M23 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.0" condition="ARMCM23 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M23 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMCM23/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM23/Source/ARM/startup_ARMCM23.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM23/Source/GCC/startup_ARMCM23.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM23/Source/GCC/gcc_arm.ld"        version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM23/Source/IAR/startup_ARMCM23.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM23/Source/system_ARMCM23.c"      version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMCM23/Include/Template/partition_ARMCM23.h" version="1.0.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.0" condition="ARMCM23 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M23 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMCM23/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM23/Source/GCC/startup_ARMCM23.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM23/Source/GCC/gcc_arm.ld"        version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM23/Source/system_ARMCM23.c"      version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMCM23/Include/Template/partition_ARMCM23.h" version="1.0.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>

    <!-- Cortex-M33 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.1.0" condition="ARMCM33 CMSIS">
      <description>System and Startup for Generic Arm Cortex-M33 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMCM33/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMCM33/Source/ARM/startup_ARMCM33.s"         version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM33/Source/GCC/startup_ARMCM33.S"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM33/Source/GCC/gcc_arm.ld"                version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCM33/Source/IAR/startup_ARMCM33.s"         version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCM33/Source/system_ARMCM33.c"              version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMCM33/Include/Template/partition_ARMCM33.h" version="1.1.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.1.0" condition="ARMCM33 CMSIS GCC">
      <description>System and Startup for Generic Arm Cortex-M33 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMCM33/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMCM33/Source/GCC/startup_ARMCM33.c"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMCM33/Source/GCC/gcc_arm.ld"                version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMCM33/Source/system_ARMCM33.c"              version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMCM33/Include/Template/partition_ARMCM33.h" version="1.1.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>

    <!-- Cortex-SC000 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMSC000 CMSIS">
      <description>System and Startup for Generic Arm SC000 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMSC000/Include/ARMSC000.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMSC000/Source/ARM/startup_ARMSC000.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMSC000/Source/GCC/startup_ARMSC000.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMSC000/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMSC000/Source/IAR/startup_ARMSC000.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMSC000/Source/system_ARMSC000.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMSC000 CMSIS GCC">
      <description>System and Startup for Generic Arm SC000 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMSC000/Include/ARMSC000.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMSC000/Source/GCC/startup_ARMSC000.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMSC000/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMSC000/Source/system_ARMSC000.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-SC300 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMSC300 CMSIS">
      <description>System and Startup for Generic Arm SC300 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMSC300/Include/ARMSC300.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMSC300/Source/ARM/startup_ARMSC300.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMSC300/Source/GCC/startup_ARMSC300.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMSC300/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMSC300/Source/IAR/startup_ARMSC300.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMSC300/Source/system_ARMSC300.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.1" condition="ARMSC300 CMSIS GCC">
      <description>System and Startup for Generic Arm SC300 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device/ARM/ARMSC300/Include/ARMSC300.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMSC300/Source/GCC/startup_ARMSC300.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMSC300/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMSC300/Source/system_ARMSC300.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- ARMv8MBL -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.0" condition="ARMv8MBL CMSIS">
      <description>System and Startup for Generic Armv8-M Baseline device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMv8MBL/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMv8MBL/Source/ARM/startup_ARMv8MBL.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMv8MBL/Source/GCC/startup_ARMv8MBL.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMv8MBL/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMv8MBL/Source/system_ARMv8MBL.c"      version="1.0.0" attr="config" condition="ARMCC GCC"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMv8MBL/Include/Template/partition_ARMv8MBL.h" version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.0.0" condition="ARMv8MBL CMSIS GCC">
      <description>System and Startup for Generic Armv8-M Baseline device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMv8MBL/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMv8MBL/Source/GCC/startup_ARMv8MBL.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMv8MBL/Source/GCC/gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMv8MBL/Source/system_ARMv8MBL.c"      version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMv8MBL/Include/Template/partition_ARMv8MBL.h" version="1.0.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>

    <!-- ARMv8MML -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.1.0" condition="ARMv8MML CMSIS">
      <description>System and Startup for Generic Armv8-M Mainline device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMv8MML/Include/"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device/ARM/ARMv8MML/Source/ARM/startup_ARMv8MML.s"         version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMv8MML/Source/GCC/startup_ARMv8MML.S"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMv8MML/Source/GCC/gcc_arm.ld"                 version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMv8MML/Source/system_ARMv8MML.c"              version="1.0.0" attr="config" condition="ARMCC GCC"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMv8MML/Include/Template/partition_ARMv8MML.h" version="1.1.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup" Cversion="1.1.0" condition="ARMv8MML CMSIS GCC">
      <description>System and Startup for Generic Armv8-M Mainline device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMv8MML/Include/"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device/ARM/ARMv8MML/Source/GCC/startup_ARMv8MML.c"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device/ARM/ARMv8MML/Source/GCC/gcc_arm.ld"                 version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device/ARM/ARMv8MML/Source/system_ARMv8MML.c"              version="1.0.0" attr="config"/>
        <!-- SAU configuration -->
        <file category="header"       name="Device/ARM/ARMv8MML/Include/Template/partition_ARMv8MML.h" version="1.1.0" attr="config" condition="ARMv8-M TZ Device"/>
      </files>
    </component>

    <!-- Cortex-A5 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.0" condition="ARMCA5 CMSIS">
      <description>System and Startup for Generic Arm Cortex-A5 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMCA5/Include/"/>
        <!-- startup / system / mmu files -->
        <file category="sourceC"      name="Device/ARM/ARMCA5/Source/AC5/startup_ARMCA5.c" version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="linkerScript" name="Device/ARM/ARMCA5/Source/AC5/ARMCA5.sct"       version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="sourceC"      name="Device/ARM/ARMCA5/Source/AC6/startup_ARMCA5.c" version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="linkerScript" name="Device/ARM/ARMCA5/Source/AC6/ARMCA5.sct"       version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="sourceC"      name="Device/ARM/ARMCA5/Source/GCC/startup_ARMCA5.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="other"        name="Device/ARM/ARMCA5/Source/GCC/ARMCA5.ld"        version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCA5/Source/IAR/startup_ARMCA5.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="linkerScript" name="Device/ARM/ARMCA5/Source/IAR/ARMCA5.icf"       version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCA5/Source/system_ARMCA5.c"      version="1.0.0" attr="config"/>
        <file category="sourceC"      name="Device/ARM/ARMCA5/Source/mmu_ARMCA5.c"         version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA5/Include/system_ARMCA5.h"     version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA5/Include/mem_ARMCA5.h"        version="1.0.0" attr="config"/>

      </files>
    </component>

    <!-- Cortex-A7 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.0" condition="ARMCA7 CMSIS">
      <description>System and Startup for Generic Arm Cortex-A7 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"      name="Device/ARM/ARMCA7/Include/"/>
        <!-- startup / system / mmu files -->
        <file category="sourceC"      name="Device/ARM/ARMCA7/Source/AC5/startup_ARMCA7.c" version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="linkerScript" name="Device/ARM/ARMCA7/Source/AC5/ARMCA7.sct"       version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="sourceC"      name="Device/ARM/ARMCA7/Source/AC6/startup_ARMCA7.c" version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="linkerScript" name="Device/ARM/ARMCA7/Source/AC6/ARMCA7.sct"       version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="sourceC"      name="Device/ARM/ARMCA7/Source/GCC/startup_ARMCA7.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="other"        name="Device/ARM/ARMCA7/Source/GCC/ARMCA7.ld"        version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCA7/Source/IAR/startup_ARMCA7.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="linkerScript" name="Device/ARM/ARMCA7/Source/IAR/ARMCA7.icf"       version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCA7/Source/system_ARMCA7.c"      version="1.0.0" attr="config"/>
        <file category="sourceC"      name="Device/ARM/ARMCA7/Source/mmu_ARMCA7.c"         version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA7/Include/system_ARMCA7.h"     version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA7/Include/mem_ARMCA7.h"        version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-A9 -->
    <component Cclass="Device" Cgroup="Startup"                      Cversion="1.0.1" condition="ARMCA9 CMSIS">
      <description>System and Startup for Generic Arm Cortex-A9 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device/ARM/ARMCA9/Include/"/>
        <!-- startup / system / mmu files -->
        <file category="sourceC"      name="Device/ARM/ARMCA9/Source/AC5/startup_ARMCA9.c" version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="linkerScript" name="Device/ARM/ARMCA9/Source/AC5/ARMCA9.sct"       version="1.0.0" attr="config" condition="ARMCC5"/>
        <file category="sourceC"      name="Device/ARM/ARMCA9/Source/AC6/startup_ARMCA9.c" version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="linkerScript" name="Device/ARM/ARMCA9/Source/AC6/ARMCA9.sct"       version="1.0.0" attr="config" condition="ARMCC6"/>
        <file category="sourceC"      name="Device/ARM/ARMCA9/Source/GCC/startup_ARMCA9.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="other"        name="Device/ARM/ARMCA9/Source/GCC/ARMCA9.ld"        version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device/ARM/ARMCA9/Source/IAR/startup_ARMCA9.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="linkerScript" name="Device/ARM/ARMCA9/Source/IAR/ARMCA9.icf"       version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device/ARM/ARMCA9/Source/system_ARMCA9.c"      version="1.0.0" attr="config"/>
        <file category="sourceC"      name="Device/ARM/ARMCA9/Source/mmu_ARMCA9.c"         version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA9/Include/system_ARMCA9.h"     version="1.0.0" attr="config"/>
        <file category="header"       name="Device/ARM/ARMCA9/Include/mem_ARMCA9.h"        version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- IRQ Controller -->
    <component Cclass="Device" Cgroup="IRQ Controller" Csub="GIC" Capiversion="1.0.0" Cversion="1.0.1" condition="ARMv7-A Device">
      <description>IRQ Controller implementation using GIC</description>
      <files>
        <file category="sourceC" name="CMSIS/Core_A/Source/irq_ctrl_gic.c"/>
      </files>
    </component>

    <!-- OS Tick -->
    <component Cclass="Device" Cgroup="OS Tick" Csub="Private Timer" Capiversion="1.0.1" Cversion="1.0.2" condition="OS Tick PTIM">
      <description>OS Tick implementation using Private Timer</description>
      <files>
        <file category="sourceC" name="CMSIS/RTOS2/Source/os_tick_ptim.c"/>
      </files>
    </component>

    <component Cclass="Device" Cgroup="OS Tick" Csub="Generic Physical Timer" Capiversion="1.0.1" Cversion="1.0.1" condition="OS Tick GTIM">
      <description>OS Tick implementation using Generic Physical Timer</description>
      <files>
        <file category="sourceC" name="CMSIS/RTOS2/Source/os_tick_gtim.c"/>
      </files>
    </component>

    <!-- CMSIS-DSP component -->
    <component Cclass="CMSIS" Cgroup="DSP" Cversion="1.5.2" condition="CMSIS DSP">
      <description>CMSIS-DSP Library for Cortex-M, SC000, and SC300</description>
      <files>
        <!-- CPU independent -->
        <file category="doc" name="CMSIS/Documentation/DSP/html/index.html"/>
        <file category="header" name="CMSIS/DSP/Include/arm_math.h"/>

        <!-- CPU and Compiler dependent -->
        <!-- ARMCC -->
        <file category="library" condition="CM0_LE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM0l_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM0_BE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM0b_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM1_LE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM0l_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM1_BE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM0b_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM3_LE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM3l_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM3_BE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM3b_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM4_LE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM4l_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM4_BE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM4b_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM4_FP_LE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM4lf_math.lib"     src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM4_FP_BE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM4bf_math.lib"     src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_LE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM7l_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_BE_ARMCC"             name="CMSIS/Lib/ARM/arm_cortexM7b_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_SP_LE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM7lfsp_math.lib"   src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_SP_BE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM7bfsp_math.lib"   src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_DP_LE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM7lfdp_math.lib"   src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM7_DP_BE_ARMCC"          name="CMSIS/Lib/ARM/arm_cortexM7bfdp_math.lib"   src="CMSIS/DSP/Source/ARM"/>

        <file category="library" condition="CM23_LE_ARMCC"                  name="CMSIS/Lib/ARM/arm_ARMv8MBLl_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM33_NODSP_NOFPU_LE_ARMCC"      name="CMSIS/Lib/ARM/arm_ARMv8MMLl_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM33_DSP_NOFPU_LE_ARMCC"        name="CMSIS/Lib/ARM/arm_ARMv8MMLld_math.lib"     src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM33_NODSP_SP_LE_ARMCC"         name="CMSIS/Lib/ARM/arm_ARMv8MMLlfsp_math.lib"   src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="CM33_DSP_SP_LE_ARMCC"           name="CMSIS/Lib/ARM/arm_ARMv8MMLldfsp_math.lib"  src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="ARMv8MBL_LE_ARMCC"              name="CMSIS/Lib/ARM/arm_ARMv8MBLl_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="ARMv8MML_NODSP_NOFPU_LE_ARMCC"  name="CMSIS/Lib/ARM/arm_ARMv8MMLl_math.lib"      src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="ARMv8MML_DSP_NOFPU_LE_ARMCC"    name="CMSIS/Lib/ARM/arm_ARMv8MMLld_math.lib"     src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="ARMv8MML_NODSP_SP_LE_ARMCC"     name="CMSIS/Lib/ARM/arm_ARMv8MMLlfsp_math.lib"   src="CMSIS/DSP/Source/ARM"/>
        <file category="library" condition="ARMv8MML_DSP_SP_LE_ARMCC"       name="CMSIS/Lib/ARM/arm_ARMv8MMLldfsp_math.lib"  src="CMSIS/DSP/Source/ARM"/>
        <!--file category="library" condition="ARMv8MML_DP_NOFPU_LE_ARMCC"     name="CMSIS/Lib/ARM/arm_ARMv8MMLlfdp_math.lib"   src="CMSIS/DSP/Source/ARM"/-->
        <!--file category="library" condition="ARMv8MML_DSP_DP_LE_ARMCC"       name="CMSIS/Lib/ARM/arm_ARMv8MMLldfdp_math.lib"  src="CMSIS/DSP/Source/ARM"/-->

        <!-- GCC -->
        <file category="library" condition="CM0_LE_GCC"               name="CMSIS/Lib/GCC/libarm_cortexM0l_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM1_LE_GCC"               name="CMSIS/Lib/GCC/libarm_cortexM0l_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM3_LE_GCC"               name="CMSIS/Lib/GCC/libarm_cortexM3l_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM4_LE_GCC"               name="CMSIS/Lib/GCC/libarm_cortexM4l_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM4_FP_LE_GCC"            name="CMSIS/Lib/GCC/libarm_cortexM4lf_math.a"    src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM7_LE_GCC"               name="CMSIS/Lib/GCC/libarm_cortexM7l_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM7_SP_LE_GCC"            name="CMSIS/Lib/GCC/libarm_cortexM7lfsp_math.a"  src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM7_DP_LE_GCC"            name="CMSIS/Lib/GCC/libarm_cortexM7lfdp_math.a"  src="CMSIS/DSP/Source/GCC"/>

        <file category="library" condition="CM23_LE_GCC"                    name="CMSIS/Lib/GCC/libarm_ARMv8MBLl_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM33_NODSP_NOFPU_LE_GCC"        name="CMSIS/Lib/GCC/libarm_ARMv8MMLl_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM33_DSP_NOFPU_LE_GCC"          name="CMSIS/Lib/GCC/libarm_ARMv8MMLld_math.a"    src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM33_NODSP_SP_LE_GCC"           name="CMSIS/Lib/GCC/libarm_ARMv8MMLlfsp_math.a"  src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="CM33_DSP_SP_LE_GCC"             name="CMSIS/Lib/GCC/libarm_ARMv8MMLldfsp_math.a" src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="ARMv8MBL_LE_GCC"                name="CMSIS/Lib/GCC/libarm_ARMv8MBLl_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="ARMv8MML_NODSP_NOFPU_LE_GCC"    name="CMSIS/Lib/GCC/libarm_ARMv8MMLl_math.a"     src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="ARMv8MML_DSP_NOFPU_LE_GCC"      name="CMSIS/Lib/GCC/libarm_ARMv8MMLld_math.a"    src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="ARMv8MML_NODSP_SP_LE_GCC"       name="CMSIS/Lib/GCC/libarm_ARMv8MMLlfsp_math.a"  src="CMSIS/DSP/Source/GCC"/>
        <file category="library" condition="ARMv8MML_DSP_SP_LE_GCC"         name="CMSIS/Lib/GCC/libarm_ARMv8MMLldfsp_math.a" src="CMSIS/DSP/Source/GCC"/>
        <!--file category="library" condition="ARMv8MML_DP_NOFPU_LE_GCC"       name="CMSIS/Lib/GCC/libarm_ARMv8MMLlfdp_math.a"  src="CMSIS/DSP/Source/GCC"/-->
        <!--file category="library" condition="ARMv8MML_DSP_DP_LE_GCC"         name="CMSIS/Lib/GCC/libarm_ARMv8MMLldfdp_math.a" src="CMSIS/DSP/Source/GCC"/-->

	<!-- IAR -->
        <file category="library" condition="CM0_LE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM0l_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM0_BE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM0b_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM1_LE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM0l_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM1_BE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM0b_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM3_LE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM3l_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM3_BE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM3b_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM4_LE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM4l_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM4_BE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM4b_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM4_FP_LE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM4lf_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM4_FP_BE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM4bf_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_LE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM7l_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_BE_IAR"               name="CMSIS/Lib/IAR/iar_cortexM7b_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_DP_LE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM7lf_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_DP_BE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM7bf_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_SP_LE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM7ls_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM7_SP_BE_IAR"            name="CMSIS/Lib/IAR/iar_cortexM7bs_math.a"    src="CMSIS/DSP/Source/IAR"/>

        <file category="library" condition="CM23_LE_IAR"              name="CMSIS/Lib/IAR/iar_ARMv8MBLl_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM33_LE_IAR"              name="CMSIS/Lib/IAR/iar_ARMv8MMLl_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM33_DSP_SP_LE_IAR"       name="CMSIS/Lib/IAR/iar_ARMv8MMLlfsp_math.a"  src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM33_FP_LE_IAR"           name="CMSIS/Lib/IAR/iar_ARMv8MMLlfdp_math.a"  src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM33_DSP_NOFPU_LE_IAR"    name="CMSIS/Lib/IAR/iar_ARMv8MMLld_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="CM33_DSP_SP_LE_IAR"       name="CMSIS/Lib/IAR/iar_ARMv8MMLldfsp_math.a" src="CMSIS/DSP/Source/IAR"/>
        <!--file category="library" condition="CM33_DSP_DP_LE_IAR"       name="CMSIS/Lib/IAR/iar_ARMv8MMLldfdp_math.a" src="CMSIS/DSP/Source/IAR"/-->
        <file category="library" condition="ARMv8MBL_LE_IAR"          name="CMSIS/Lib/IAR/iar_ARMv8MBLl_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="ARMv8MML_LE_IAR"          name="CMSIS/Lib/IAR/iar_ARMv8MMLl_math.a"     src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="ARMv8MML_DSP_SP_LE_IAR"   name="CMSIS/Lib/IAR/iar_ARMv8MMLlfsp_math.a"  src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="ARMv8MML_FP_LE_IAR"       name="CMSIS/Lib/IAR/iar_ARMv8MMLlfdp_math.a"  src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="ARMv8MML_DSP_NOFPU_LE_IAR" name="CMSIS/Lib/IAR/iar_ARMv8MMLld_math.a"    src="CMSIS/DSP/Source/IAR"/>
        <file category="library" condition="ARMv8MML_DSP_SP_LE_IAR"   name="CMSIS/Lib/IAR/iar_ARMv8MMLldfsp_math.a" src="CMSIS/DSP/Source/IAR"/>
        <!--file category="library" condition="ARMv8MML_DSP_DP_LE_IAR"   name="CMSIS/Lib/IAR/iar_ARMv8MMLldfdp_math.a" src="CMSIS/DSP/Source/IAR"/-->

      </files>
    </component>

    <!-- CMSIS-NN component -->
    <component Cclass="CMSIS" Cgroup="NN Lib" Cversion="1.1.0" condition="CMSIS NN">
      <description>CMSIS-NN Neural Network Library</description>
      <files>
        <file category="doc" name="CMSIS/Documentation/NN/html/index.html"/>
        <file category="header" name="CMSIS/NN/Include/arm_nnfunctions.h"/>

        <file category="source" name="CMSIS/NN/Source/ActivationFunctions/arm_nn_activations_q7.c"/>
        <file category="source" name="CMSIS/NN/Source/ActivationFunctions/arm_nn_activations_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/ActivationFunctions/arm_relu_q7.c"/>
        <file category="source" name="CMSIS/NN/Source/ActivationFunctions/arm_relu_q15.c"/>

        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q7_RGB.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q15_basic.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q15_fast.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_depthwise_separable_conv_HWC_q7.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_depthwise_separable_conv_HWC_q7_nonsquare.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_nn_mat_mult_kernel_q7_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_nn_mat_mult_kernel_q7_q15_reordered.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_1x1_HWC_q7_fast_nonsquare.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q7_basic.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q7_basic_nonsquare.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q7_fast.c"/>
        <file category="source" name="CMSIS/NN/Source/ConvolutionFunctions/arm_convolve_HWC_q7_fast_nonsquare.c"/>

        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_q7.c"/>
        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_q7_opt.c"/>
        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_q15_opt.c"/>
        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_mat_q7_vec_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/FullyConnectedFunctions/arm_fully_connected_mat_q7_vec_q15_opt.c"/>

        <file category="source" name="CMSIS/NN/Source/NNSupportFunctions/arm_q7_to_q15_reordered_no_shift.c"/>
        <file category="source" name="CMSIS/NN/Source/NNSupportFunctions/arm_nntables.c"/>
        <file category="source" name="CMSIS/NN/Source/NNSupportFunctions/arm_q7_to_q15_no_shift.c"/>
        <file category="source" name="CMSIS/NN/Source/NNSupportFunctions/arm_nn_mult_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/NNSupportFunctions/arm_nn_mult_q7.c"/>

        <file category="source" name="CMSIS/NN/Source/PoolingFunctions/arm_pool_q7_HWC.c"/>

        <file category="source" name="CMSIS/NN/Source/SoftmaxFunctions/arm_softmax_q15.c"/>
        <file category="source" name="CMSIS/NN/Source/SoftmaxFunctions/arm_softmax_q7.c"/>
      </files>
    </component>

    <!-- CMSIS-RTOS Keil RTX component -->
    <component Cclass="CMSIS" Cgroup="RTOS" Csub="Keil RTX" Cversion="4.81.1" Capiversion="1.0.0" isDefaultVariant="1" condition="RTOS RTX">
      <description>CMSIS-RTOS RTX implementation for Cortex-M, SC000, and SC300</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS                  /* CMSIS-RTOS */
        #define RTE_CMSIS_RTOS_RTX              /* CMSIS-RTOS Keil RTX */
      </RTE_Components_h>
      <files>
        <!-- CPU independent -->
        <file category="doc" name="CMSIS/Documentation/RTOS/html/rtxImplementation.html"/>
        <file category="header" name="CMSIS/RTOS/RTX/INC/cmsis_os.h"/>
        <file category="source" attr="config"   name="CMSIS/RTOS/RTX/Templates/RTX_Conf_CM.c" version="4.70.1"/>

        <!-- RTX templates -->
        <file category="header" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/osObjects.h" select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/main.c"      select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MailQueue.c" select="CMSIS-RTOS Mail Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MemPool.c"   select="CMSIS-RTOS Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MsgQueue.c"  select="CMSIS-RTOS Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Mutex.c"     select="CMSIS-RTOS Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Semaphore.c" select="CMSIS-RTOS Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Thread.c"    select="CMSIS-RTOS Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Timer.c"     select="CMSIS-RTOS Timer"/>
        <!-- tool-chain specific template file -->
        <file category="source" attr="template" condition="ARMCC" name="CMSIS/RTOS/RTX/SRC/ARM/SVC_Table.s" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="GCC"   name="CMSIS/RTOS/RTX/SRC/GCC/SVC_Table.S" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="IAR"   name="CMSIS/RTOS/RTX/SRC/IAR/SVC_Table.s" select="CMSIS-RTOS User SVC"/>

        <!-- CPU and Compiler dependent -->
        <!-- ARMCC -->
        <file category="library" condition="CM0_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM0.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM0_BE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM0_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM1_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM0.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM1_BE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM0_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM3_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM3_BE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM4_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM4_BE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM4_FP_LE_ARMCC" name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM4.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM4_FP_BE_ARMCC" name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM4_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM7_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM7_BE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM7_FP_LE_ARMCC" name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM4.lib"    src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM7_FP_BE_ARMCC" name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM4_B.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <!-- GCC -->
        <file category="library" condition="CM0_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM0.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM0_BE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM0_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM1_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM0.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM1_BE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM0_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM3_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM3_BE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM4_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM4_BE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM4_FP_LE_GCC"   name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM4.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM4_FP_BE_GCC"   name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM4_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM7_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM7_BE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM7_FP_LE_GCC"   name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM4.a"   src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM7_FP_BE_GCC"   name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM4_B.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <!-- IAR -->
        <file category="library" condition="CM0_LE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM0.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM0_BE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM0_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM1_LE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM0.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM1_BE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM0_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM3_LE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM3_BE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM4_LE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM4_BE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM4_FP_LE_IAR"   name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM4.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM4_FP_BE_IAR"   name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM4_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM7_LE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM7_BE_IAR"      name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM3_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM7_FP_LE_IAR"   name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM4.a"      src="CMSIS/RTOS/RTX/SRC/IAR"/>
        <file category="library" condition="CM7_FP_BE_IAR"   name="CMSIS/RTOS/RTX/LIB/IAR/RTX_CM4_B.a"    src="CMSIS/RTOS/RTX/SRC/IAR"/>
      </files>
    </component>
    <!-- CMSIS-RTOS Keil RTX component (IFX variant) -->
    <component Cclass="CMSIS" Cgroup="RTOS" Csub="Keil RTX" Cvariant="IFX" Cversion="4.81.1" Capiversion="1.0.0" condition="RTOS RTX IFX">
      <description>CMSIS-RTOS RTX implementation for Infineon XMC4 series affected by PMU_CM.001 errata</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS                  /* CMSIS-RTOS */
        #define RTE_CMSIS_RTOS_RTX              /* CMSIS-RTOS Keil RTX */
      </RTE_Components_h>
      <files>
        <!-- CPU independent -->
        <file category="doc" name="CMSIS/Documentation/RTOS/html/rtxImplementation.html"/>
        <file category="header" name="CMSIS/RTOS/RTX/INC/cmsis_os.h"/>
        <file category="source" attr="config"   name="CMSIS/RTOS/RTX/Templates/RTX_Conf_CM.c" version="4.70.1"/>

        <!-- RTX templates -->
        <file category="header" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/osObjects.h" select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/main.c"      select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MailQueue.c" select="CMSIS-RTOS Mail Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MemPool.c"   select="CMSIS-RTOS Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/MsgQueue.c"  select="CMSIS-RTOS Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Mutex.c"     select="CMSIS-RTOS Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Semaphore.c" select="CMSIS-RTOS Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Thread.c"    select="CMSIS-RTOS Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS/RTX/UserCodeTemplates/Timer.c"     select="CMSIS-RTOS Timer"/>
        <!-- tool-chain specific template file -->
        <file category="source" attr="template" condition="ARMCC" name="CMSIS/RTOS/RTX/SRC/ARM/SVC_Table.s" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="GCC"   name="CMSIS/RTOS/RTX/SRC/GCC/SVC_Table.S" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="IAR"   name="CMSIS/RTOS/RTX/SRC/IAR/SVC_Table.s" select="CMSIS-RTOS User SVC"/>

        <!-- CPU and Compiler dependent -->
        <!-- ARMCC -->
        <file category="library" condition="CM4_LE_ARMCC"    name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM3_IFX.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <file category="library" condition="CM4_FP_LE_ARMCC" name="CMSIS/RTOS/RTX/LIB/ARM/RTX_CM4_IFX.lib"  src="CMSIS/RTOS/RTX/SRC/ARM"/>
        <!-- GCC -->
        <file category="library" condition="CM4_LE_GCC"      name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM3_IFX.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <file category="library" condition="CM4_FP_LE_GCC"   name="CMSIS/RTOS/RTX/LIB/GCC/libRTX_CM4_IFX.a" src="CMSIS/RTOS/RTX/SRC/GCC"/>
        <!-- IAR -->
      </files>
    </component>

    <!-- CMSIS-RTOS Keil RTX5 component -->
    <component Cclass="CMSIS" Cgroup="RTOS" Csub="Keil RTX5" Cversion="5.4.0" Capiversion="1.0.0" condition="RTOS RTX5">
      <description>CMSIS-RTOS RTX5 implementation for Cortex-M, SC000, and SC300</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS                  /* CMSIS-RTOS */
        #define RTE_CMSIS_RTOS_RTX5             /* CMSIS-RTOS Keil RTX5 */
      </RTE_Components_h>
      <files>
        <!-- RTX header file -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include1/cmsis_os.h"/>
        <!-- RTX compatibility module for API V1 -->
        <file category="source" name="CMSIS/RTOS2/RTX/Library/cmsis_os1.c"/>
      </files>
    </component>

    <!-- CMSIS-RTOS2 Keil RTX5 component -->
    <component Cclass="CMSIS" Cgroup="RTOS2" Csub="Keil RTX5" Cvariant="Library" Cversion="5.4.0" Capiversion="2.1.3" condition="RTOS2 RTX5 Lib">
      <description>CMSIS-RTOS2 RTX5 for Cortex-M, SC000, C300 and Armv8-M (Library)</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS2                 /* CMSIS-RTOS2 */
        #define RTE_CMSIS_RTOS2_RTX5            /* CMSIS-RTOS2 Keil RTX5 */
      </RTE_Components_h>
      <files>
        <!-- RTX documentation -->
        <file category="doc"    name="CMSIS/Documentation/RTOS2/html/rtx5_impl.html"/>

        <!-- RTX header files -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include/rtx_os.h"/>

        <!-- RTX configuration -->
        <file category="header" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.h"  version="5.4.0"/>
        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.c"  version="5.1.0"/>

        <!-- RTX templates -->
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/main.c"      version="2.0.0" select="CMSIS-RTOS2 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Events.c"    version="2.0.0" select="CMSIS-RTOS2 Events"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MemPool.c"   version="2.0.0" select="CMSIS-RTOS2 Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MsgQueue.c"  version="2.0.0" select="CMSIS-RTOS2 Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Mutex.c"     version="2.0.0" select="CMSIS-RTOS2 Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Semaphore.c" version="2.0.0" select="CMSIS-RTOS2 Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Thread.c"    version="2.0.0" select="CMSIS-RTOS2 Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Timer.c"     version="2.0.1" select="CMSIS-RTOS2 Timer"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/svc_user.c"  version="1.0.0" select="CMSIS-RTOS2 SVC User Table"/>
        <file category="other"  name="CMSIS/RTOS2/RTX/RTX5.scvd"/>

        <!-- RTX library configuration -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_lib.c"/>

        <!-- RTX libraries (CPU and Compiler dependent) -->
        <!-- ARMCC -->
        <file category="library" condition="CM0_LE_ARMCC"         name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM0.lib"    src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM1_LE_ARMCC"         name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM0.lib"    src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM3_LE_ARMCC"         name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM3.lib"    src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_LE_ARMCC"         name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM3.lib"    src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_FP_LE_ARMCC"      name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM4F.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_LE_ARMCC"         name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM3.lib"    src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_FP_LE_ARMCC"      name="CMSIS/RTOS2/RTX/Library/ARM/RTX_CM4F.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM23_LE_ARMCC"        name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MB.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_LE_ARMCC"        name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MM.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_FP_LE_ARMCC"     name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMF.lib"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MBL_LE_ARMCC"    name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MB.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_LE_ARMCC"    name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MM.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_FP_LE_ARMCC" name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMF.lib"  src="CMSIS/RTOS2/RTX/Source"/>
        <!-- GCC -->
        <file category="library" condition="CM0_LE_GCC"           name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM0.a"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM1_LE_GCC"           name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM0.a"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM3_LE_GCC"           name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM3.a"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_LE_GCC"           name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM3.a"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_FP_LE_GCC"        name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM4F.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_LE_GCC"           name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM3.a"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_FP_LE_GCC"        name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_CM4F.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM23_LE_GCC"          name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MB.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_LE_GCC"          name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MM.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_FP_LE_GCC"       name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMF.a" src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MBL_LE_GCC"      name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MB.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_LE_GCC"      name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MM.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_FP_LE_GCC"   name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMF.a" src="CMSIS/RTOS2/RTX/Source"/>
        <!-- IAR -->
        <file category="library" condition="CM0_LE_IAR"           name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM0.a"      src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM1_LE_IAR"           name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM0.a"      src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM3_LE_IAR"           name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM3.a"      src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_LE_IAR"           name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM3.a"      src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM4_FP_LE_IAR"        name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM4F.a"     src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_LE_IAR"           name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM3.a"      src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM7_FP_LE_IAR"        name="CMSIS/RTOS2/RTX/Library/IAR/RTX_CM4F.a"     src="CMSIS/RTOS2/RTX/Source"/>
      </files>
    </component>
    <component Cclass="CMSIS" Cgroup="RTOS2" Csub="Keil RTX5" Cvariant="Library_NS" Cversion="5.4.0" Capiversion="2.1.3" condition="RTOS2 RTX5 NS">
      <description>CMSIS-RTOS2 RTX5 for Armv8-M Non-Secure Domain (Library)</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS2                 /* CMSIS-RTOS2 */
        #define RTE_CMSIS_RTOS2_RTX5            /* CMSIS-RTOS2 Keil RTX5 */
        #define RTE_CMSIS_RTOS2_RTX5_ARMV8M_NS  /* CMSIS-RTOS2 Keil RTX5 Armv8-M Non-secure domain */
      </RTE_Components_h>
      <files>
        <!-- RTX documentation -->
        <file category="doc"    name="CMSIS/Documentation/RTOS2/html/rtx5_impl.html"/>

        <!-- RTX header files -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include/rtx_os.h"/>

        <!-- RTX configuration -->
        <file category="header" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.h"  version="5.4.0"/>
        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.c"  version="5.1.0"/>

        <!-- RTX templates -->
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/main.c"      version="2.0.0" select="CMSIS-RTOS2 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Events.c"    version="2.0.0" select="CMSIS-RTOS2 Events"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MemPool.c"   version="2.0.0" select="CMSIS-RTOS2 Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MsgQueue.c"  version="2.0.0" select="CMSIS-RTOS2 Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Mutex.c"     version="2.0.0" select="CMSIS-RTOS2 Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Semaphore.c" version="2.0.0" select="CMSIS-RTOS2 Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Thread.c"    version="2.0.0" select="CMSIS-RTOS2 Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Timer.c"     version="2.0.1" select="CMSIS-RTOS2 Timer"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/svc_user.c"  version="1.0.0" select="CMSIS-RTOS2 SVC User Table"/>
        <file category="other"  name="CMSIS/RTOS2/RTX/RTX5.scvd"/>

        <!-- RTX library configuration -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_lib.c"/>

        <!-- RTX libraries (CPU and Compiler dependent) -->
        <!-- ARMCC -->
        <file category="library" condition="CM23_LE_ARMCC"        name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MBN.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_LE_ARMCC"        name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMN.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_FP_LE_ARMCC"     name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMFN.lib"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MBL_LE_ARMCC"    name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MBN.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_LE_ARMCC"    name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMN.lib"   src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_FP_LE_ARMCC" name="CMSIS/RTOS2/RTX/Library/ARM/RTX_V8MMFN.lib"  src="CMSIS/RTOS2/RTX/Source"/>
        <!-- GCC -->
        <file category="library" condition="CM23_LE_GCC"          name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MBN.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_LE_GCC"          name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMN.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="CM33_FP_LE_GCC"       name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMFN.a" src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MBL_LE_GCC"      name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MBN.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_LE_GCC"      name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMN.a"  src="CMSIS/RTOS2/RTX/Source"/>
        <file category="library" condition="ARMv8MML_FP_LE_GCC"   name="CMSIS/RTOS2/RTX/Library/GCC/libRTX_V8MMFN.a" src="CMSIS/RTOS2/RTX/Source"/>
      </files>
    </component>
    <component Cclass="CMSIS" Cgroup="RTOS2" Csub="Keil RTX5" Cvariant="Source" Cversion="5.4.0" Capiversion="2.1.3" condition="RTOS2 RTX5">
      <description>CMSIS-RTOS2 RTX5 for Cortex-M, SC000, C300 and Armv8-M (Source)</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS2                 /* CMSIS-RTOS2 */
        #define RTE_CMSIS_RTOS2_RTX5            /* CMSIS-RTOS2 Keil RTX5 */
        #define RTE_CMSIS_RTOS2_RTX5_SOURCE     /* CMSIS-RTOS2 Keil RTX5 Source */
      </RTE_Components_h>
      <files>
        <!-- RTX documentation -->
        <file category="doc"    name="CMSIS/Documentation/RTOS2/html/rtx5_impl.html"/>

        <!-- RTX header files -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include/rtx_os.h"/>

        <!-- RTX configuration -->
        <file category="header" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.h"  version="5.4.0"/>
        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.c"  version="5.1.0"/>

        <!-- RTX templates -->
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/main.c"      version="2.0.0" select="CMSIS-RTOS2 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Events.c"    version="2.0.0" select="CMSIS-RTOS2 Events"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MemPool.c"   version="2.0.0" select="CMSIS-RTOS2 Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MsgQueue.c"  version="2.0.0" select="CMSIS-RTOS2 Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Mutex.c"     version="2.0.0" select="CMSIS-RTOS2 Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Semaphore.c" version="2.0.0" select="CMSIS-RTOS2 Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Thread.c"    version="2.0.0" select="CMSIS-RTOS2 Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Timer.c"     version="2.0.1" select="CMSIS-RTOS2 Timer"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/svc_user.c"  version="1.0.0" select="CMSIS-RTOS2 SVC User Table"/>
        <file category="other"  name="CMSIS/RTOS2/RTX/RTX5.scvd"/>

        <!-- RTX sources (core) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_kernel.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_thread.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_delay.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_timer.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evflags.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mutex.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_semaphore.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_memory.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mempool.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_msgqueue.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_system.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evr.c"/>
        <!-- RTX sources (library configuration) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_lib.c"/>
        <!-- RTX sources (handlers ARMCC) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm0.s"         condition="CM0_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm0.s"         condition="CM1_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm3.s"         condition="CM3_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm3.s"         condition="CM4_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm4f.s"        condition="CM4_FP_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm3.s"         condition="CM7_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_cm4f.s"        condition="CM7_FP_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mbl.s"    condition="CM23_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml.s"    condition="CM33_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml.s"    condition="CM33_FP_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mbl.s"    condition="ARMv8MBL_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml.s"    condition="ARMv8MML_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml.s"    condition="ARMv8MML_FP_ARMCC"/>
        <!-- RTX sources (handlers GCC) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm0.S"         condition="CM0_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm0.S"         condition="CM1_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm3.S"         condition="CM3_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm3.S"         condition="CM4_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm4f.S"        condition="CM4_FP_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm3.S"         condition="CM7_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_cm4f.S"        condition="CM7_FP_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mbl.S"    condition="CM23_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml.S"    condition="CM33_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_fp.S" condition="CM33_FP_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mbl.S"    condition="ARMv8MBL_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml.S"    condition="ARMv8MML_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_fp.S" condition="ARMv8MML_FP_GCC"/>
        <!-- RTX sources (handlers IAR) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm0.s"         condition="CM0_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm0.s"         condition="CM1_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm3.s"         condition="CM3_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm3.s"         condition="CM4_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm4f.s"        condition="CM4_FP_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm3.s"         condition="CM7_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_cm4f.s"        condition="CM7_FP_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mbl.s"    condition="CM23_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml.s"    condition="CM33_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml.s"    condition="CM33_FP_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mbl.s"    condition="ARMv8MBL_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml.s"    condition="ARMv8MML_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml.s"    condition="ARMv8MML_FP_IAR"/>
        <!-- OS Tick (SysTick) -->
        <file category="source" name="CMSIS/RTOS2/Source/os_systick.c"/>
      </files>
    </component>
    <component Cclass="CMSIS" Cgroup="RTOS2" Csub="Keil RTX5" Cvariant="Source" Cversion="5.4.0" Capiversion="2.1.3" condition="RTOS2 RTX5 v7-A">
      <description>CMSIS-RTOS2 RTX5 for Armv7-A (Source)</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS2                 /* CMSIS-RTOS2 */
        #define RTE_CMSIS_RTOS2_RTX5            /* CMSIS-RTOS2 Keil RTX5 */
        #define RTE_CMSIS_RTOS2_RTX5_SOURCE     /* CMSIS-RTOS2 Keil RTX5 Source */
      </RTE_Components_h>
      <files>
        <!-- RTX documentation -->
        <file category="doc"    name="CMSIS/Documentation/RTOS2/html/rtx5_impl.html"/>

        <!-- RTX header files -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include/rtx_os.h"/>

        <!-- RTX configuration -->
        <file category="header" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.h"  version="5.4.0"/>
        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.c"  version="5.1.0"/>

        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/handlers.c"    version="5.1.0"/>

        <!-- RTX templates -->
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/main.c"      version="2.0.0" select="CMSIS-RTOS2 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Events.c"    version="2.0.0" select="CMSIS-RTOS2 Events"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MemPool.c"   version="2.0.0" select="CMSIS-RTOS2 Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MsgQueue.c"  version="2.0.0" select="CMSIS-RTOS2 Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Mutex.c"     version="2.0.0" select="CMSIS-RTOS2 Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Semaphore.c" version="2.0.0" select="CMSIS-RTOS2 Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Thread.c"    version="2.0.0" select="CMSIS-RTOS2 Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Timer.c"     version="2.0.1" select="CMSIS-RTOS2 Timer"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/svc_user.c"  version="1.0.0" select="CMSIS-RTOS2 SVC User Table"/>
        <file category="other"  name="CMSIS/RTOS2/RTX/RTX5.scvd"/>

        <!-- RTX sources (core) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_kernel.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_thread.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_delay.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_timer.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evflags.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mutex.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_semaphore.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_memory.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mempool.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_msgqueue.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_system.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evr.c"/>
        <!-- RTX sources (library configuration) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_lib.c"/>
        <!-- RTX sources (handlers ARMCC) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_ca.s"          condition="CA_ARMCC5"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_ca.S"          condition="CA_ARMCC6"/>
        <!-- RTX sources (handlers GCC) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_ca.S"          condition="CA_GCC"/>
        <!-- RTX sources (handlers IAR) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_ca.s"          condition="CA_IAR"/>
      </files>
    </component>
    <component Cclass="CMSIS" Cgroup="RTOS2" Csub="Keil RTX5" Cvariant="Source_NS" Cversion="5.4.0" Capiversion="2.1.3" condition="RTOS2 RTX5 NS">
      <description>CMSIS-RTOS2 RTX5 for Armv8-M Non-Secure Domain (Source)</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS2                 /* CMSIS-RTOS2 */
        #define RTE_CMSIS_RTOS2_RTX5            /* CMSIS-RTOS2 Keil RTX5 */
        #define RTE_CMSIS_RTOS2_RTX5_SOURCE     /* CMSIS-RTOS2 Keil RTX5 Source */
        #define RTE_CMSIS_RTOS2_RTX5_ARMV8M_NS  /* CMSIS-RTOS2 Keil RTX5 Armv8-M Non-secure domain */
      </RTE_Components_h>
      <files>
        <!-- RTX documentation -->
        <file category="doc"    name="CMSIS/Documentation/RTOS2/html/rtx5_impl.html"/>

        <!-- RTX header files -->
        <file category="header" name="CMSIS/RTOS2/RTX/Include/rtx_os.h"/>

        <!-- RTX configuration -->
        <file category="header" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.h"  version="5.4.0"/>
        <file category="source" attr="config"   name="CMSIS/RTOS2/RTX/Config/RTX_Config.c"  version="5.1.0"/>

        <!-- RTX templates -->
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/main.c"      version="2.0.0" select="CMSIS-RTOS2 'main' function"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Events.c"    version="2.0.0" select="CMSIS-RTOS2 Events"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MemPool.c"   version="2.0.0" select="CMSIS-RTOS2 Memory Pool"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/MsgQueue.c"  version="2.0.0" select="CMSIS-RTOS2 Message Queue"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Mutex.c"     version="2.0.0" select="CMSIS-RTOS2 Mutex"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Semaphore.c" version="2.0.0" select="CMSIS-RTOS2 Semaphore"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Thread.c"    version="2.0.0" select="CMSIS-RTOS2 Thread"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/Timer.c"     version="2.0.1" select="CMSIS-RTOS2 Timer"/>
        <file category="source" attr="template" name="CMSIS/RTOS2/RTX/Template/svc_user.c"  version="1.0.0" select="CMSIS-RTOS2 SVC User Table"/>
        <file category="other"  name="CMSIS/RTOS2/RTX/RTX5.scvd"/>

        <!-- RTX sources (core) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_kernel.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_thread.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_delay.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_timer.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evflags.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mutex.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_semaphore.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_memory.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_mempool.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_msgqueue.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_system.c"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_evr.c"/>
        <!-- RTX sources (library configuration) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/rtx_lib.c"/>
        <!-- RTX sources (ARMCC handlers) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mbl_ns.s"    condition="CM23_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml_ns.s"    condition="CM33_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml_ns.s"    condition="CM33_FP_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mbl_ns.s"    condition="ARMv8MBL_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml_ns.s"    condition="ARMv8MML_ARMCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/ARM/irq_armv8mml_ns.s"    condition="ARMv8MML_FP_ARMCC"/>
        <!-- RTX sources (GCC handlers) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mbl_ns.S"    condition="CM23_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_ns.S"    condition="CM33_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_fp_ns.S" condition="CM33_FP_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mbl_ns.S"    condition="ARMv8MBL_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_ns.S"    condition="ARMv8MML_GCC"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/GCC/irq_armv8mml_fp_ns.S" condition="ARMv8MML_FP_GCC"/>
        <!-- RTX sources (IAR handlers) -->
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mbl_ns.s"    condition="CM23_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml_ns.s"    condition="CM33_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml_ns.s"    condition="CM33_FP_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mbl_ns.s"    condition="ARMv8MBL_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml_ns.s"    condition="ARMv8MML_IAR"/>
        <file category="source" name="CMSIS/RTOS2/RTX/Source/IAR/irq_armv8mml_ns.s"    condition="ARMv8MML_FP_IAR"/>
        <!-- OS Tick (SysTick) -->
        <file category="source" name="CMSIS/RTOS2/Source/os_systick.c"/>
      </files>
    </component>

  </components>

  <boards>
    <board name="uVision Simulator" vendor="Keil">
      <description>uVision Simulator</description>
      <mountedDevice    deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM0"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM0P"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM0P_MPU"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM1"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM3"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM4"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM4_FP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM7"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM7_SP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM7_DP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMv8MBL"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMv8MML"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMv8MML_SP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMv8MML_DP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM23"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM23_TZ"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM33"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM33_TZ"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM33_DSP_FP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM33_DSP_FP_TZ"/>
    </board>

    <board name="Fixed Virtual Platform" vendor="ARM">
      <description>Fixed Virtual Platform</description>
      <mountedDevice    deviceIndex="0" Dvendor="ARM:82" Dname="ARMCA5"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCA7"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCA9"/>
    </board>
  </boards>

  <examples>
    <example name="DSP_Lib Class Marks example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_class_marks_example">
      <description>DSP_Lib Class Marks example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_class_marks_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Convolution example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_convolution_example">
      <description>DSP_Lib Convolution example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_convolution_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Dotproduct example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_dotproduct_example">
      <description>DSP_Lib Dotproduct example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_dotproduct_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib FFT Bin example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_fft_bin_example">
      <description>DSP_Lib FFT Bin example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_fft_bin_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib FIR example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_fir_example">
      <description>DSP_Lib FIR example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_fir_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Graphic Equalizer example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_graphic_equalizer_example">
      <description>DSP_Lib Graphic Equalizer example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_graphic_equalizer_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Linear Interpolation example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_linear_interp_example">
      <description>DSP_Lib Linear Interpolation example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_linear_interp_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Matrix example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_matrix_example">
      <description>DSP_Lib Matrix example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_matrix_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Signal Convergence example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_signal_converge_example">
      <description>DSP_Lib Signal Convergence example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_signal_converge_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Sinus/Cosinus example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_sin_cos_example">
      <description>DSP_Lib Sinus/Cosinus example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_sin_cos_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Variance example" doc="Abstract.txt" folder="CMSIS/DSP/Examples/ARM/arm_variance_example">
      <description>DSP_Lib Variance example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_variance_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="NN Library CIFAR10" doc="readme.txt" folder="CMSIS/NN/Examples/ARM/arm_nn_examples/cifar10">
      <description>Neural Network CIFAR10 example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_nnexamples_cifar10.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="CMSIS" Cgroup="NN Lib"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="NN Library GRU" doc="readme.txt" folder="CMSIS/NN/Examples/ARM/arm_nn_examples/gru">
      <description>Neural Network GRU example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_nnexamples_gru.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="CMSIS" Cgroup="NN Lib"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="CMSIS-RTOS2 Blinky" doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/Blinky">
      <description>CMSIS-RTOS2 Blinky example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="Blinky.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="CMSIS-RTOS2 RTX5 Migration" doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/Migration">
      <description>CMSIS-RTOS2 mixed API v1 and v2</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="Blinky.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="CMSIS-RTOS2 RTX5 Message Queue" doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/MsgQueue">
      <description>CMSIS-RTOS2 Message Queue Example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="MsqQueue.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Compiler" Cgroup="EventRecorder"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="CMSIS-RTOS2 RTX5 Memory Pool" doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/MemPool">
      <description>CMSIS-RTOS2 Memory Pool Example</description>
      <board name="Fixed Virtual Platform" vendor="ARM"/>
      <project>
        <environment name="uv" load="MemPool.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Compiler" Cgroup="EventRecorder"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="TrustZone for ARMv8-M No RTOS" doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/TrustZoneV8M/NoRTOS">
      <description>Bare-metal secure/non-secure example without RTOS</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="NoRTOS.uvmpw"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="TrustZone for ARMv8-M RTOS"  doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/TrustZoneV8M/RTOS">
      <description>Secure/non-secure RTOS example with thread context management</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="RTOS.uvmpw"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="TrustZone for ARMv8-M RTOS Security Tests"  doc="Abstract.txt" folder="CMSIS/RTOS2/RTX/Examples/TrustZoneV8M/RTOS_Faults">
      <description>Secure/non-secure RTOS example with security test cases and system recovery</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="RTOS_Faults.uvmpw"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="RTOS2"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

  </examples>

</package>
