================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了COMP比较器轮询功能，PD0作为比较器正端输入，1/2Vrebuf2.048V作为比较器
负端输入，当PD0的电压大于1/2Vrebuf2.048V电压时，LED灯亮，小于1/2Vrebuf2.048V电
压时,LED灯灭。

Function descriptions:
This example demonstrates the COMP comparator polling function, with PD0 as the 
positive input and 1/2Vrebuf2.048V as the negative input. When the voltage of
PD0 is greater than 1/2Vrebuf2.048V voltage, the LED lights up, and when it is
less than 1/2Vrebuf2.048V voltage, the LED lights off.

================================================================================
测试环境：
测试用板：PY32L090_STK
MDK版本： 5.28
IAR版本： 9.20
GCC版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32L090_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 配置PD0输入1.0V电压，LED灯灭;
3. 配置PD0输入1.05V电压, LED灯亮;

Example execution steps:
1.Compile and download the program to MCU and run it;
2.Configure PD0 input voltage of 1.0V, LED light off;
3.Configure PD0 input voltage of 1.05V, LED light on;

================================================================================
注意事项：

Notes:

================================================================================